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Figure S1. Results of antimicrobial susceptibility testing for 43 Gram-negative isolates obtained from the second fecal samples
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Figure S2. Results of antimicrobial susceptibility testing for 18 Gram-negative isolates obtained from the third fecal sample



[image: ]
Figure S3. Results of antimicrobial susceptibility testing for 29 E. coli isolates obtained from the second fecal samples
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Figure S4. Results of antimicrobial susceptibility testing for 10 E. coli isolates obtained from the third fecal sample
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Figure S5. Comparative assessment for antibiotic resistance rate between E. coli and ‎K. pneumoniae ‎spp.‎ obtained from fecal samples
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Figure S6. Co-occurrence of Resistance Genes
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Antimicrobial susceptibility test results of 10 E. coli strain recovered from the third fecal sampling
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