Additional File 1:  MRI settings per scanner type
	MRI sequence
	Settings

	
	Philips 3T 
	GE 3T
	Siemens 3T

	3DT1
	Sagittal 3D turbo field echo sequence (1.00 mm isotropic voxels, TR = 7.9 ms, TE = 4.5 ms, FA = 8 degrees)
	Sagittal 3D FSPGR   (1.00 mm isotropic voxels, TR = 8.2 ms, TE = 3.2 ms / TI = 450 ms, FA = 12 degrees)

	3D MPRAGE (1.00 mm x 1.00 mm x 1.00 mm voxels, TR = 2300 ms, TE = 3 ms)

	3D Fluid-attenuated inversion recovery
	3D sagittal VISTA sequence (1.12 mm isotropic voxels, TR = 4800 ms, TE = 279 ms, inversion time = 1650 ms)
	3D sagittal CUBE sequence (1.2 mm isotropic voxels, TR = 8000 ms, TE = 130 ms, inversion time = 2340 ms)
	3D sagittal SPACE sequence (1.2 mm isptropic voxels, TR = 5000 ms, TE = 387 ms ms, inversion time = 2340 ms)

	2D PD-T2: 

	Oblique axial orientation, 45-48 slices of 3mm thickness (TR = 3925 ms, TE = 19 and 100 ms)
	Oblique axial orientation, 45-48 slices of 3mm thickness (TR = 8600 ms, TE = 20 and 112 ms) 
	Oblique axial orientation, 45-48 slices of 3mm thickness (TR = 4730 ms, TE = 20 ms)


TR: repetition time; TE: echo time; FA: flip angle.
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