Preoperative CT-based deep learning radiomics model to predict lymph node metastasis and patient prognosis in bladder cancer: a two-center study

ELECTRONIC SUPPLEMENTARY MATERIAL
Table S1 CT acquisition settings.
	Parameters
	The Affiliated Hospital of Qingdao University
	Shandong Provincial Hospital Affiliated to Shandong First Medical University

	CT equipment
	BrightSpeed RT 16 Elite; Aquilion ONE 640, TOSHIBA; LightSpeed CT750 HD, GE Healthcare; SOMATOM CT, Siemens Healthcare; Somatom Sensation Cardiac 64, Siemens Healthcare; Brilliance iCT, Philips Healthcare;
	Discovery 750, GE Healthcare; Somatom Definition Flash, Siemens Healthcare; Aquilion ONE, TOSHIBA

	Matrix size
	512 × 512
	512 × 512

	Tube current
	automatic tube current modulation
	automatic tube current modulation

	Pitch
	0.8
	0.8

	Tube voltage
	120 kV
	120 kV

	Slice thickness
	5mm
	5mm

	Detector collimation
	64×0.6mm
or 64×0.625mm
	64×0.6mm
or 64×0.625mm

	Contrast agent
	Ultravist 370
or Omnipaque 350
	Omnipaque 350

	Injection rate
	3.0ml/s
	3.0ml/s

	Contrast medium dose
	80~90ml
	80~90ml
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