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[image: ]Raw, continuous lava flow-substrate heat transfer results from when lava first inundates the location of interest through to nine months after the end of the emplacement period.
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