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	ICP-AES
	Properties

	RF power
	0.7-1.8 Kw (1.2-1.3 kW for axial)

	Auxilary gas flow rate (Ar)
	1.5

	Plasma gas flow rate (Pr)
	10.5-15 L/min (radial), 15 “(axial)”

	Copy time
	3 s (max. 100 s)

	Copy and reading time
	1-5 s (max. 60 s)

	Viewing height
	5-12 mm





