Summary tables of net depth measurements
These tables provide summaries of the bottom (leadline) and breastline depths measured for 11 nets deployed in the ESSN fishing district in 2015.  Summaries are provided at several levels: 1) for each time-depth recorder on each net, 2) for each Site; and 3) for all nets combined.  TDR=serial number of the time-depth recorder; SE=standard error; SD=standard deviation. Percentiles indicate the depths that includes the first n percent of the total depth measurements when sorted in ascending order (here n = 0, 10, 25, 50, 75, 90, and 100%).
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	Site
	Mesh
	Replicate
	TDR
	Tidal hour
	Count
	Mean
	SE
	SD
	Min
	10%
	25%
	Median
	75%
	90%
	Max

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	one
	13904
	1
	1603
	2.87
	0.02
	0.65
	1.42
	1.71
	2.47
	3.04
	3.39
	3.60
	3.80

	
	
	
	
	2
	1776
	1.68
	0.01
	0.54
	0.90
	1.08
	1.24
	1.57
	2.03
	2.38
	3.43

	
	
	
	
	3
	1831
	0.81
	0.00
	0.10
	0.65
	0.70
	0.73
	0.79
	0.87
	0.97
	1.10

	
	
	
	
	4
	1831
	0.83
	0.00
	0.10
	0.67
	0.73
	0.76
	0.80
	0.93
	0.98
	1.06

	
	
	
	
	5
	1831
	0.92
	0.00
	0.12
	0.74
	0.79
	0.82
	0.90
	1.01
	1.10
	1.25

	
	
	
	
	6
	1718
	1.24
	0.01
	0.22
	0.84
	0.90
	1.07
	1.29
	1.38
	1.47
	1.71

	
	
	
	
	7
	1757
	2.09
	0.01
	0.49
	1.45
	1.60
	1.72
	1.91
	2.40
	2.85
	3.55

	
	
	
	
	8
	1080
	3.00
	0.02
	0.81
	1.43
	1.76
	2.21
	3.33
	3.73
	3.95
	4.01

	
	
	
	
	9
	423
	1.12
	0.01
	0.24
	0.77
	0.81
	0.85
	1.17
	1.33
	1.42
	1.57

	
	
	
	
	10
	389
	0.61
	0.01
	0.13
	0.44
	0.49
	0.50
	0.56
	0.68
	0.81
	0.91

	
	
	
	
	11
	421
	1.16
	0.01
	0.19
	0.74
	0.81
	1.04
	1.23
	1.28
	1.32
	1.47

	
	
	
	
	12
	778
	1.81
	0.02
	0.47
	1.18
	1.29
	1.39
	1.70
	2.25
	2.49
	2.86

	
	
	
	
	13
	1415
	3.04
	0.02
	0.77
	1.22
	1.45
	2.69
	3.23
	3.65
	3.85
	4.10

	
	
	
	
	14
	2053
	1.63
	0.01
	0.66
	0.51
	0.83
	1.08
	1.56
	2.10
	2.63
	3.13

	
	
	
	
	15
	2085
	0.92
	0.01
	0.27
	0.43
	0.49
	0.84
	0.93
	1.00
	1.35
	1.62

	
	
	
	
	16
	2114
	0.98
	0.01
	0.24
	0.51
	0.54
	0.90
	1.00
	1.18
	1.28
	1.33

	
	
	
	
	17
	2114
	1.03
	0.01
	0.27
	0.55
	0.57
	0.91
	1.03
	1.26
	1.40
	1.56

	
	
	
	
	18
	2136
	1.26
	0.01
	0.32
	0.58
	0.67
	1.12
	1.25
	1.50
	1.65
	1.93

	
	
	
	
	19
	2130
	2.04
	0.01
	0.60
	1.13
	1.35
	1.62
	1.96
	2.34
	2.81
	3.83

	
	
	
	
	20
	2081
	3.10
	0.02
	0.75
	1.19
	1.93
	2.55
	3.20
	3.74
	3.94
	4.98

	
	
	
	
	21
	1708
	1.66
	0.01
	0.54
	0.34
	1.04
	1.31
	1.56
	2.00
	2.48
	2.94

	
	
	
	
	22
	1945
	1.03
	0.01
	0.46
	0.33
	0.37
	0.89
	0.96
	1.28
	1.78
	1.91

	
	
	
	
	23
	2009
	1.06
	0.01
	0.46
	0.37
	0.39
	0.84
	1.02
	1.18
	1.80
	2.03

	
	
	
	
	24
	1952
	1.50
	0.01
	0.60
	0.49
	0.67
	1.17
	1.37
	1.91
	2.45
	3.00

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	two
	13908
	1
	1665
	3.62
	0.00
	0.19
	2.98
	3.36
	3.56
	3.68
	3.73
	3.77
	3.88

	
	
	
	
	2
	1780
	2.84
	0.01
	0.48
	1.99
	2.21
	2.42
	2.78
	3.25
	3.51
	3.73

	
	
	
	
	3
	1831
	1.77
	0.00
	0.15
	1.51
	1.61
	1.68
	1.73
	1.86
	2.02
	2.21

	
	
	
	
	4
	1831
	1.80
	0.00
	0.16
	1.51
	1.60
	1.69
	1.78
	1.88
	2.06
	2.16

	
	
	
	
	5
	1831
	1.96
	0.00
	0.17
	1.55
	1.74
	1.86
	1.98
	2.07
	2.16
	2.32

	
	
	
	
	6
	1660
	2.42
	0.01
	0.30
	1.83
	1.99
	2.16
	2.41
	2.70
	2.80
	3.07

	
	
	
	
	7
	1750
	3.12
	0.01
	0.31
	2.48
	2.76
	2.86
	3.09
	3.33
	3.64
	3.79

	
	
	
	
	8
	1091
	3.57
	0.01
	0.25
	2.89
	3.15
	3.39
	3.72
	3.74
	3.76
	3.85

	
	
	
	
	9
	424
	2.36
	0.02
	0.39
	1.73
	1.81
	1.92
	2.47
	2.71
	2.85
	2.97

	
	
	
	
	10
	389
	1.40
	0.02
	0.45
	0.95
	0.97
	1.04
	1.16
	1.79
	2.10
	2.33

	
	
	
	
	11
	421
	2.66
	0.02
	0.36
	2.02
	2.09
	2.46
	2.69
	2.88
	3.11
	3.48

	
	
	
	
	12
	780
	3.10
	0.01
	0.37
	2.51
	2.59
	2.74
	3.13
	3.48
	3.55
	3.68

	
	
	
	
	13
	1477
	3.72
	0.00
	0.11
	3.22
	3.59
	3.71
	3.73
	3.77
	3.80
	3.96

	
	
	
	
	14
	2025
	2.94
	0.01
	0.66
	1.79
	2.13
	2.47
	2.87
	3.35
	3.75
	4.99

	
	
	
	
	15
	2085
	1.98
	0.01
	0.26
	1.50
	1.63
	1.76
	2.01
	2.20
	2.26
	2.60

	
	
	
	
	16
	2114
	2.08
	0.01
	0.27
	1.63
	1.72
	1.92
	2.02
	2.27
	2.55
	2.69

	
	
	
	
	17
	2114
	2.15
	0.01
	0.28
	1.70
	1.82
	1.93
	2.11
	2.29
	2.61
	2.82

	
	
	
	
	18
	2109
	2.43
	0.01
	0.27
	1.91
	2.14
	2.23
	2.37
	2.64
	2.84
	3.10

	
	
	
	
	19
	2133
	3.10
	0.01
	0.40
	2.22
	2.52
	2.89
	3.11
	3.42
	3.66
	3.77

	
	
	
	
	20
	2114
	3.61
	0.01
	0.27
	2.68
	3.13
	3.52
	3.73
	3.77
	3.82
	3.93

	
	
	
	
	21
	1710
	2.87
	0.01
	0.46
	1.50
	2.33
	2.62
	2.84
	3.19
	3.52
	3.76

	
	
	
	
	22
	1945
	2.23
	0.01
	0.36
	1.51
	1.61
	2.03
	2.29
	2.54
	2.62
	2.82

	
	
	
	
	23
	2009
	2.37
	0.01
	0.32
	1.77
	1.89
	2.15
	2.35
	2.64
	2.80
	3.02

	
	
	
	
	24
	1954
	2.89
	0.01
	0.37
	2.24
	2.38
	2.61
	2.89
	3.16
	3.44
	3.70

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	three
	13893
	1
	0
	NA
	NA
	NA
	0
	0
	0
	0
	0
	0
	0

	
	
	
	
	2
	0
	NA
	NA
	NA
	0
	0
	0
	0
	0
	0
	0

	
	
	
	
	3
	272
	1.24
	0.00
	0.05
	1.18
	1.19
	1.20
	1.21
	1.27
	1.33
	1.40

	
	
	
	
	4
	345
	1.15
	0.00
	0.06
	1.04
	1.07
	1.12
	1.15
	1.21
	1.23
	1.25

	
	
	
	
	5
	345
	1.16
	0.00
	0.06
	1.06
	1.08
	1.10
	1.15
	1.21
	1.24
	1.25

	
	
	
	
	6
	367
	1.42
	0.01
	0.11
	1.24
	1.28
	1.31
	1.42
	1.52
	1.57
	1.62

	
	
	
	
	7
	329
	2.16
	0.03
	0.58
	1.61
	1.68
	1.79
	1.99
	2.27
	3.64
	3.69

	
	
	
	
	8
	142
	3.72
	0.00
	0.04
	3.65
	3.67
	3.68
	3.71
	3.76
	3.77
	3.78

	
	
	
	
	9
	0
	NA
	NA
	NA
	0
	0
	0
	0
	0
	0
	0

	
	
	
	
	10
	0
	NA
	NA
	NA
	0
	0
	0
	0
	0
	0
	0

	
	
	
	
	11
	0
	NA
	NA
	NA
	0
	0
	0
	0
	0
	0
	0

	
	
	
	
	12
	69
	2.81
	0.00
	0.03
	2.77
	2.78
	2.80
	2.80
	2.81
	2.84
	2.90

	
	
	
	
	13
	468
	2.90
	0.01
	0.19
	1.72
	2.85
	2.87
	2.91
	2.99
	3.04
	3.18

	
	
	
	
	14
	931
	2.34
	0.01
	0.34
	1.60
	1.81
	2.11
	2.41
	2.61
	2.74
	2.85

	
	
	
	
	15
	1012
	1.62
	0.01
	0.19
	1.30
	1.36
	1.45
	1.62
	1.75
	1.87
	2.19

	
	
	
	
	16
	832
	1.43
	0.01
	0.15
	1.16
	1.24
	1.29
	1.44
	1.58
	1.60
	1.72

	
	
	
	
	17
	1012
	1.41
	0.01
	0.19
	1.16
	1.22
	1.25
	1.33
	1.63
	1.69
	1.74

	
	
	
	
	18
	884
	1.69
	0.01
	0.28
	1.08
	1.31
	1.47
	1.67
	1.88
	2.07
	2.28

	
	
	
	
	19
	1173
	2.43
	0.01
	0.32
	1.86
	1.94
	2.19
	2.42
	2.70
	2.85
	3.00

	
	
	
	
	20
	1173
	2.96
	0.01
	0.26
	2.48
	2.66
	2.79
	2.92
	3.08
	3.41
	3.53

	
	
	
	
	21
	1173
	2.54
	0.01
	0.50
	1.68
	1.79
	2.04
	2.56
	2.95
	3.17
	3.46

	
	
	
	
	22
	1173
	1.96
	0.01
	0.24
	1.60
	1.65
	1.69
	1.97
	2.16
	2.27
	2.42

	
	
	
	
	23
	450
	1.90
	0.00
	0.07
	1.76
	1.79
	1.84
	1.90
	1.96
	1.99
	2.02

	
	
	
	
	24
	240
	2.53
	0.01
	0.10
	2.29
	2.40
	2.46
	2.54
	2.63
	2.66
	2.68

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	four
	13895
	1
	874
	2.70
	0.01
	0.19
	2.14
	2.37
	2.66
	2.76
	2.85
	2.89
	2.96

	
	
	
	
	2
	1112
	2.28
	0.01
	0.25
	1.83
	1.92
	2.10
	2.28
	2.45
	2.62
	2.81

	
	
	
	
	3
	1415
	1.85
	0.00
	0.16
	1.48
	1.67
	1.72
	1.86
	1.94
	2.01
	2.46

	
	
	
	
	4
	1458
	1.69
	0.00
	0.19
	1.44
	1.47
	1.50
	1.67
	1.80
	2.00
	2.13

	
	
	
	
	5
	1458
	1.72
	0.00
	0.13
	1.51
	1.55
	1.60
	1.73
	1.78
	1.95
	2.00

	
	
	
	
	6
	1305
	2.02
	0.01
	0.24
	1.56
	1.64
	1.85
	2.03
	2.22
	2.33
	2.56

	
	
	
	
	7
	1132
	2.73
	0.01
	0.32
	2.30
	2.38
	2.47
	2.64
	2.92
	3.28
	3.31

	
	
	
	
	8
	539
	2.77
	0.01
	0.24
	2.12
	2.38
	2.75
	2.83
	2.89
	2.95
	3.35

	
	
	
	
	9
	647
	1.78
	0.01
	0.15
	1.59
	1.61
	1.63
	1.75
	1.92
	1.99
	2.12

	
	
	
	
	10
	808
	1.78
	0.01
	0.21
	1.44
	1.51
	1.59
	1.89
	1.98
	2.02
	2.09

	
	
	
	
	11
	1037
	2.15
	0.01
	0.36
	1.68
	1.71
	1.81
	2.23
	2.48
	2.60
	2.87

	
	
	
	
	12
	1338
	2.78
	0.01
	0.50
	1.84
	1.88
	2.59
	3.02
	3.12
	3.20
	3.33

	
	
	
	
	13
	1408
	3.09
	0.01
	0.44
	1.94
	2.16
	3.21
	3.28
	3.33
	3.37
	3.48

	
	
	
	
	14
	2365
	2.50
	0.01
	0.47
	1.70
	1.91
	2.07
	2.44
	2.96
	3.15
	3.22

	
	
	
	
	15
	2476
	1.86
	0.01
	0.35
	1.32
	1.44
	1.60
	1.79
	2.09
	2.40
	2.73

	
	
	
	
	16
	2356
	2.08
	0.01
	0.62
	1.37
	1.48
	1.56
	1.87
	2.33
	3.08
	3.71

	
	
	
	
	17
	2476
	2.28
	0.01
	0.71
	1.43
	1.51
	1.72
	1.99
	2.90
	3.42
	3.92

	
	
	
	
	18
	2379
	1.99
	0.01
	0.47
	1.41
	1.54
	1.62
	1.83
	2.22
	2.76
	3.71

	
	
	
	
	19
	2208
	2.68
	0.01
	0.45
	1.44
	2.11
	2.33
	2.66
	3.13
	3.26
	3.33

	
	
	
	
	20
	1833
	3.19
	0.00
	0.20
	2.61
	2.88
	3.18
	3.25
	3.30
	3.33
	3.43

	
	
	
	
	21
	1408
	2.98
	0.01
	0.33
	2.24
	2.49
	2.66
	3.08
	3.29
	3.34
	3.40

	
	
	
	
	22
	1347
	2.49
	0.01
	0.25
	2.01
	2.09
	2.31
	2.49
	2.73
	2.82
	3.00

	
	
	
	
	23
	763
	2.27
	0.01
	0.20
	2.00
	2.04
	2.10
	2.25
	2.43
	2.58
	2.64

	
	
	
	
	24
	1018
	2.61
	0.01
	0.21
	2.28
	2.39
	2.44
	2.56
	2.79
	2.95
	3.12

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	45 mesh
	one
	13889
	1
	1119
	3.43
	0.03
	0.91
	1.79
	2.00
	2.69
	3.65
	3.94
	4.50
	5.28

	
	
	
	
	2
	1317
	1.54
	0.02
	0.77
	0.59
	0.76
	0.89
	1.33
	2.03
	2.67
	5.24

	
	
	
	
	3
	1831
	0.60
	0.00
	0.14
	0.32
	0.38
	0.53
	0.59
	0.71
	0.76
	1.02

	
	
	
	
	4
	1831
	0.60
	0.00
	0.13
	0.35
	0.41
	0.53
	0.58
	0.68
	0.81
	0.84

	
	
	
	
	5
	1831
	0.70
	0.00
	0.17
	0.37
	0.48
	0.59
	0.69
	0.83
	0.96
	1.04

	
	
	
	
	6
	1666
	1.03
	0.01
	0.34
	0.45
	0.60
	0.77
	1.01
	1.25
	1.47
	1.78

	
	
	
	
	7
	1148
	2.16
	0.02
	0.77
	0.74
	1.32
	1.69
	2.08
	2.56
	3.32
	4.45

	
	
	
	
	8
	575
	3.90
	0.04
	1.06
	1.74
	2.25
	2.95
	4.32
	4.83
	5.00
	5.16

	
	
	
	
	9
	389
	1.12
	0.02
	0.31
	0.68
	0.71
	0.80
	1.15
	1.32
	1.58
	1.73

	
	
	
	
	10
	389
	0.80
	0.01
	0.24
	0.45
	0.53
	0.55
	0.79
	1.07
	1.11
	1.16

	
	
	
	
	11
	451
	1.38
	0.01
	0.29
	0.77
	0.79
	1.16
	1.50
	1.57
	1.62
	1.79

	
	
	
	
	12
	718
	1.37
	0.02
	0.62
	0.80
	0.84
	0.94
	1.14
	1.63
	2.10
	4.06

	
	
	
	
	13
	1054
	2.73
	0.04
	1.36
	0.74
	1.20
	1.55
	2.33
	3.81
	4.89
	5.45

	
	
	
	
	14
	1875
	1.25
	0.01
	0.63
	0.24
	0.36
	0.96
	1.18
	1.48
	2.17
	3.23

	
	
	
	
	15
	2114
	0.68
	0.01
	0.23
	0.18
	0.24
	0.59
	0.74
	0.84
	0.93
	1.13

	
	
	
	
	16
	2114
	0.66
	0.00
	0.21
	0.20
	0.26
	0.62
	0.72
	0.77
	0.82
	1.11

	
	
	
	
	17
	2114
	0.77
	0.01
	0.27
	0.23
	0.29
	0.68
	0.80
	0.91
	1.13
	1.31

	
	
	
	
	18
	1957
	1.01
	0.01
	0.39
	0.26
	0.33
	0.81
	1.06
	1.28
	1.45
	1.80

	
	
	
	
	19
	2069
	2.01
	0.02
	0.72
	0.38
	1.19
	1.32
	1.92
	2.73
	3.02
	3.70

	
	
	
	
	20
	1845
	3.63
	0.03
	1.34
	0.57
	1.69
	2.64
	3.79
	4.81
	5.29
	5.65

	
	
	
	
	21
	1542
	1.37
	0.02
	0.74
	0.22
	0.36
	0.91
	1.45
	1.83
	2.29
	3.70

	
	
	
	
	22
	1867
	0.82
	0.01
	0.36
	0.22
	0.26
	0.54
	0.80
	1.14
	1.28
	1.45

	
	
	
	
	23
	1902
	1.08
	0.01
	0.49
	0.34
	0.61
	0.77
	0.98
	1.23
	1.73
	3.38

	
	
	
	
	24
	1952
	1.68
	0.01
	0.40
	1.00
	1.15
	1.42
	1.65
	1.88
	2.31
	2.80

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	45 mesh
	two
	13890
	1
	1093
	4.61
	0.02
	0.80
	2.65
	3.20
	4.42
	4.99
	5.17
	5.30
	5.34

	
	
	
	
	2
	1319
	3.09
	0.03
	1.24
	0.70
	1.06
	2.32
	2.99
	4.05
	4.88
	5.27

	
	
	
	
	3
	1831
	1.47
	0.01
	0.47
	0.58
	0.62
	1.36
	1.59
	1.74
	1.99
	2.39

	
	
	
	
	4
	1831
	1.46
	0.01
	0.43
	0.61
	0.64
	1.45
	1.64
	1.74
	1.84
	1.96

	
	
	
	
	5
	1831
	1.67
	0.01
	0.54
	0.58
	0.67
	1.69
	1.86
	2.01
	2.18
	2.35

	
	
	
	
	6
	1605
	2.36
	0.02
	0.98
	0.64
	0.72
	1.92
	2.59
	3.10
	3.53
	3.74

	
	
	
	
	7
	1177
	4.02
	0.03
	1.08
	0.81
	3.27
	3.68
	4.16
	4.78
	5.21
	5.34

	
	
	
	
	8
	545
	5.15
	0.02
	0.49
	3.64
	4.38
	5.02
	5.33
	5.38
	5.70
	5.83

	
	
	
	
	9
	389
	2.46
	0.03
	0.60
	1.55
	1.66
	1.77
	2.49
	2.85
	3.35
	3.63

	
	
	
	
	10
	389
	1.95
	0.04
	0.78
	0.93
	1.02
	1.08
	2.02
	2.82
	2.90
	3.02

	
	
	
	
	11
	447
	3.23
	0.02
	0.51
	2.10
	2.20
	2.91
	3.38
	3.55
	3.73
	4.00

	
	
	
	
	12
	722
	3.44
	0.03
	0.72
	2.25
	2.45
	2.86
	3.47
	3.89
	4.44
	5.27

	
	
	
	
	13
	1024
	5.01
	0.01
	0.27
	3.78
	4.66
	4.89
	5.04
	5.18
	5.29
	5.45

	
	
	
	
	14
	1876
	3.39
	0.02
	0.78
	2.12
	2.43
	2.72
	3.29
	3.99
	4.53
	5.13

	
	
	
	
	15
	2114
	1.90
	0.01
	0.34
	1.36
	1.47
	1.62
	1.83
	2.14
	2.33
	2.87

	
	
	
	
	16
	2114
	1.83
	0.01
	0.25
	1.37
	1.56
	1.63
	1.73
	2.04
	2.15
	2.50

	
	
	
	
	17
	2114
	2.11
	0.01
	0.33
	1.47
	1.72
	1.81
	2.16
	2.36
	2.59
	2.79

	
	
	
	
	18
	1943
	2.68
	0.01
	0.45
	1.89
	2.09
	2.34
	2.66
	2.98
	3.38
	3.71

	
	
	
	
	19
	2085
	4.15
	0.01
	0.64
	2.67
	3.29
	3.68
	4.15
	4.70
	5.01
	5.30

	
	
	
	
	20
	1875
	5.16
	0.01
	0.31
	3.95
	4.77
	5.07
	5.25
	5.33
	5.38
	5.85

	
	
	
	
	21
	1542
	3.49
	0.02
	0.79
	1.94
	2.32
	3.03
	3.50
	4.07
	4.49
	5.31

	
	
	
	
	22
	1868
	2.17
	0.01
	0.56
	1.16
	1.56
	1.73
	1.97
	2.71
	2.93
	3.40

	
	
	
	
	23
	1901
	2.37
	0.01
	0.47
	1.55
	1.79
	1.93
	2.37
	2.74
	2.93
	4.49

	
	
	
	
	24
	1915
	3.17
	0.02
	0.74
	1.90
	2.42
	2.63
	2.96
	3.65
	4.26
	5.01

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	45 mesh
	three
	13891
	1
	1832
	5.56
	0.01
	0.55
	3.42
	4.89
	5.35
	5.63
	5.74
	5.83
	7.19

	
	
	
	
	2
	1698
	4.08
	0.02
	1.02
	2.39
	2.87
	3.20
	3.96
	4.88
	5.58
	6.07

	
	
	
	
	3
	1831
	2.15
	0.01
	0.31
	1.68
	1.75
	1.89
	2.07
	2.38
	2.54
	3.08

	
	
	
	
	4
	1831
	2.11
	0.01
	0.26
	1.75
	1.82
	1.92
	2.01
	2.28
	2.55
	2.68

	
	
	
	
	5
	1771
	2.41
	0.01
	0.29
	1.98
	2.07
	2.14
	2.41
	2.61
	2.76
	3.47

	
	
	
	
	6
	1695
	3.21
	0.01
	0.44
	2.24
	2.58
	2.93
	3.22
	3.53
	3.77
	4.21

	
	
	
	
	7
	1389
	4.63
	0.02
	0.73
	3.39
	3.65
	3.89
	4.90
	5.22
	5.54
	5.74

	
	
	
	
	8
	723
	5.50
	0.02
	0.47
	4.49
	4.73
	5.19
	5.59
	5.78
	6.07
	6.33

	
	
	
	
	9
	389
	3.21
	0.03
	0.66
	2.26
	2.48
	2.55
	3.19
	3.83
	4.20
	4.49

	
	
	
	
	10
	389
	2.46
	0.03
	0.64
	1.69
	1.86
	2.01
	2.16
	2.64
	3.61
	3.80

	
	
	
	
	11
	329
	3.74
	0.01
	0.15
	3.48
	3.54
	3.58
	3.74
	3.87
	3.93
	4.00

	
	
	
	
	12
	463
	4.10
	0.01
	0.31
	3.49
	3.67
	3.95
	4.09
	4.21
	4.53
	4.91

	
	
	
	
	13
	747
	5.28
	0.02
	0.57
	4.19
	4.42
	4.93
	5.28
	5.69
	6.05
	6.35

	
	
	
	
	14
	1870
	3.89
	0.02
	0.76
	2.45
	2.95
	3.28
	3.86
	4.43
	5.12
	5.56

	
	
	
	
	15
	2114
	2.35
	0.01
	0.42
	1.62
	1.82
	2.04
	2.29
	2.68
	2.95
	3.47

	
	
	
	
	16
	2114
	2.13
	0.01
	0.36
	1.54
	1.84
	1.91
	2.03
	2.23
	2.87
	3.06

	
	
	
	
	17
	2114
	2.37
	0.01
	0.39
	1.84
	2.02
	2.09
	2.22
	2.59
	3.00
	3.45

	
	
	
	
	18
	2138
	2.98
	0.01
	0.48
	2.10
	2.36
	2.51
	2.99
	3.36
	3.62
	3.94

	
	
	
	
	19
	1831
	4.35
	0.02
	0.64
	2.86
	3.50
	3.94
	4.34
	4.82
	5.17
	5.68

	
	
	
	
	20
	1904
	5.57
	0.01
	0.36
	4.21
	5.14
	5.30
	5.66
	5.80
	6.00
	6.31

	
	
	
	
	21
	1198
	4.38
	0.02
	0.73
	3.18
	3.36
	3.90
	4.23
	4.90
	5.59
	5.84

	
	
	
	
	22
	1559
	3.14
	0.01
	0.58
	1.75
	2.03
	3.01
	3.35
	3.59
	3.67
	3.81

	
	
	
	
	23
	1641
	3.29
	0.01
	0.46
	2.15
	2.57
	2.92
	3.38
	3.67
	3.83
	4.15

	
	
	
	
	24
	1890
	4.51
	0.02
	0.79
	2.91
	3.65
	4.01
	4.38
	4.90
	5.36
	7.00

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site B
	29 mesh
	one
	13842
	1
	2046
	2.43
	0.03
	1.34
	0.00
	0.01
	1.75
	3.20
	3.37
	3.47
	3.73

	
	
	
	
	2
	2604
	1.75
	0.01
	0.54
	0.28
	0.90
	1.46
	1.86
	2.12
	2.40
	2.81

	
	
	
	
	3
	2728
	1.65
	0.01
	0.30
	1.09
	1.17
	1.39
	1.74
	1.87
	2.06
	2.11

	
	
	
	
	4
	3024
	1.64
	0.01
	0.31
	1.08
	1.22
	1.33
	1.73
	1.92
	2.06
	2.16

	
	
	
	
	5
	3024
	1.91
	0.01
	0.39
	1.28
	1.41
	1.59
	1.92
	2.17
	2.43
	3.08

	
	
	
	
	6
	2683
	2.76
	0.01
	0.46
	0.68
	2.19
	2.46
	2.81
	3.16
	3.30
	3.46

	
	
	
	
	7
	2499
	3.02
	0.01
	0.41
	2.01
	2.35
	2.72
	3.15
	3.37
	3.42
	3.60

	
	
	
	
	8
	2200
	1.92
	0.01
	0.31
	1.42
	1.53
	1.69
	1.89
	2.06
	2.31
	2.96

	
	
	
	
	9
	1863
	1.74
	0.00
	0.16
	1.42
	1.45
	1.70
	1.80
	1.84
	1.88
	2.04

	
	
	
	
	10
	1802
	1.73
	0.01
	0.27
	0.47
	1.48
	1.56
	1.81
	1.90
	2.02
	2.14

	
	
	
	
	11
	1859
	1.55
	0.02
	0.78
	-0.02
	0.00
	1.61
	1.91
	2.04
	2.16
	2.25

	
	
	
	
	12
	1621
	2.34
	0.02
	0.62
	-0.12
	1.56
	2.07
	2.44
	2.69
	3.06
	3.39

	
	
	
	
	13
	1496
	3.27
	0.01
	0.26
	2.36
	2.83
	3.20
	3.35
	3.44
	3.50
	3.62

	
	
	
	
	14
	1146
	1.97
	0.01
	0.37
	1.52
	1.57
	1.71
	1.89
	2.13
	2.38
	3.37

	
	
	
	
	15
	1080
	1.61
	0.01
	0.20
	1.32
	1.36
	1.46
	1.53
	1.79
	1.91
	1.94

	
	
	
	
	16
	1137
	1.47
	0.00
	0.17
	1.25
	1.29
	1.33
	1.40
	1.66
	1.70
	1.78

	
	
	
	
	17
	1344
	1.61
	0.01
	0.34
	1.21
	1.28
	1.34
	1.47
	1.77
	2.23
	2.38

	
	
	
	
	18
	1332
	2.39
	0.02
	0.61
	1.42
	1.59
	1.90
	2.38
	3.00
	3.23
	3.45

	
	
	
	
	19
	1193
	2.85
	0.02
	0.57
	1.92
	2.06
	2.20
	3.06
	3.38
	3.44
	3.65

	
	
	
	
	20
	748
	1.77
	0.01
	0.16
	1.51
	1.56
	1.70
	1.75
	1.83
	2.00
	2.30

	
	
	
	
	21
	748
	1.66
	0.00
	0.11
	1.44
	1.49
	1.57
	1.71
	1.76
	1.78
	1.81

	
	
	
	
	22
	1122
	1.38
	0.01
	0.32
	0.55
	0.92
	1.31
	1.41
	1.48
	1.64
	2.18

	
	
	
	
	23
	1526
	1.38
	0.02
	0.79
	0.01
	0.02
	0.54
	1.54
	2.17
	2.28
	2.52

	
	
	
	
	24
	1625
	1.94
	0.03
	1.19
	0.00
	0.01
	1.58
	2.51
	2.89
	3.21
	3.40

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site B
	29 mesh
	two
	13847
	1
	1380
	2.42
	0.02
	0.82
	0.92
	1.03
	1.73
	2.66
	3.14
	3.31
	3.45

	
	
	
	
	2
	1237
	1.88
	0.01
	0.27
	1.41
	1.57
	1.64
	1.85
	2.14
	2.23
	2.58

	
	
	
	
	3
	1245
	1.71
	0.01
	0.24
	1.39
	1.49
	1.54
	1.57
	1.97
	2.05
	2.13

	
	
	
	
	4
	1510
	1.66
	0.01
	0.24
	1.36
	1.39
	1.43
	1.55
	1.95
	2.00
	2.09

	
	
	
	
	5
	1317
	1.76
	0.01
	0.42
	1.35
	1.39
	1.45
	1.67
	1.82
	2.30
	3.12

	
	
	
	
	6
	1134
	2.70
	0.02
	0.67
	1.43
	1.69
	2.07
	3.17
	3.28
	3.34
	3.50

	
	
	
	
	7
	1294
	2.82
	0.01
	0.43
	2.02
	2.19
	2.51
	2.77
	3.23
	3.38
	3.52

	
	
	
	
	8
	1063
	2.03
	0.01
	0.29
	1.58
	1.62
	1.77
	2.04
	2.21
	2.45
	2.73

	
	
	
	
	9
	842
	1.88
	0.01
	0.21
	1.45
	1.54
	1.74
	1.83
	2.09
	2.13
	2.19

	
	
	
	
	10
	715
	2.02
	0.01
	0.28
	1.71
	1.73
	1.75
	1.81
	2.30
	2.36
	2.45

	
	
	
	
	11
	677
	2.20
	0.01
	0.37
	1.76
	1.78
	1.85
	1.98
	2.61
	2.67
	2.68

	
	
	
	
	12
	649
	2.52
	0.01
	0.24
	2.02
	2.11
	2.48
	2.50
	2.57
	2.85
	3.09

	
	
	
	
	13
	739
	2.72
	0.01
	0.30
	2.15
	2.36
	2.54
	2.65
	2.87
	3.23
	3.41

	
	
	
	
	14
	752
	2.11
	0.02
	0.42
	1.59
	1.61
	1.69
	2.13
	2.46
	2.71
	2.95

	
	
	
	
	15
	409
	1.86
	0.01
	0.18
	1.54
	1.61
	1.79
	1.81
	1.84
	2.18
	2.21

	
	
	
	
	16
	379
	1.77
	0.00
	0.01
	1.75
	1.76
	1.77
	1.77
	1.78
	1.79
	1.80

	
	
	
	
	17
	380
	1.80
	0.00
	0.02
	1.77
	1.77
	1.78
	1.79
	1.82
	1.84
	1.85

	
	
	
	
	18
	317
	2.42
	0.03
	0.52
	1.83
	1.86
	1.97
	2.17
	3.01
	3.19
	3.27

	
	
	
	
	19
	371
	3.23
	0.01
	0.26
	2.55
	2.76
	3.07
	3.34
	3.43
	3.46
	3.47

	
	
	
	
	20
	0
	NA
	NA
	NA
	0
	0
	0
	0
	0
	0
	0

	
	
	
	
	21
	325
	1.57
	0.02
	0.35
	1.18
	1.29
	1.32
	1.36
	2.06
	2.13
	2.18

	
	
	
	
	22
	656
	1.49
	0.01
	0.15
	1.27
	1.32
	1.35
	1.43
	1.66
	1.68
	1.79

	
	
	
	
	23
	756
	1.66
	0.01
	0.14
	1.42
	1.48
	1.52
	1.67
	1.76
	1.85
	1.95

	
	
	
	
	24
	843
	2.48
	0.02
	0.45
	0.91
	2.14
	2.36
	2.56
	2.70
	2.92
	3.16

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site B
	29 mesh
	three
	13866
	1
	3145
	2.87
	0.01
	0.60
	1.24
	1.98
	2.51
	3.02
	3.40
	3.51
	3.60

	
	
	
	
	2
	2818
	1.81
	0.01
	0.71
	0.92
	0.98
	1.29
	1.68
	2.23
	3.03
	3.52

	
	
	
	
	3
	2761
	1.38
	0.01
	0.29
	0.84
	0.89
	1.15
	1.34
	1.61
	1.78
	1.87

	
	
	
	
	4
	2667
	1.29
	0.00
	0.25
	0.82
	0.91
	1.07
	1.33
	1.39
	1.71
	1.79

	
	
	
	
	5
	2667
	1.57
	0.01
	0.41
	0.94
	1.04
	1.36
	1.48
	1.75
	2.14
	2.92

	
	
	
	
	6
	2187
	2.78
	0.01
	0.67
	1.39
	1.85
	2.17
	3.02
	3.44
	3.49
	3.61

	
	
	
	
	7
	2955
	2.41
	0.01
	0.64
	1.32
	1.60
	1.84
	2.35
	2.97
	3.36
	3.53

	
	
	
	
	8
	3287
	1.42
	0.00
	0.16
	1.17
	1.23
	1.29
	1.39
	1.49
	1.66
	2.05

	
	
	
	
	9
	3100
	1.20
	0.00
	0.12
	0.73
	1.08
	1.15
	1.20
	1.29
	1.35
	1.42

	
	
	
	
	10
	3373
	1.25
	0.00
	0.11
	0.89
	1.10
	1.16
	1.25
	1.33
	1.40
	1.51

	
	
	
	
	11
	3297
	1.44
	0.00
	0.14
	1.15
	1.27
	1.35
	1.44
	1.52
	1.65
	1.76

	
	
	
	
	12
	3756
	1.82
	0.01
	0.60
	0.67
	0.84
	1.52
	1.86
	2.20
	2.53
	3.30

	
	
	
	
	13
	4116
	2.53
	0.01
	0.77
	0.78
	1.39
	2.00
	2.57
	3.25
	3.49
	3.71

	
	
	
	
	14
	4266
	1.66
	0.01
	0.38
	1.14
	1.30
	1.46
	1.56
	1.76
	2.04
	3.35

	
	
	
	
	15
	4474
	1.45
	0.01
	0.35
	1.12
	1.21
	1.28
	1.41
	1.49
	1.63
	3.47

	
	
	
	
	16
	4476
	1.34
	0.00
	0.15
	1.10
	1.16
	1.22
	1.30
	1.41
	1.58
	1.90

	
	
	
	
	17
	4302
	1.56
	0.01
	0.33
	1.11
	1.20
	1.29
	1.50
	1.68
	2.06
	2.60

	
	
	
	
	18
	3723
	3.00
	0.01
	0.53
	1.38
	2.10
	2.71
	3.17
	3.43
	3.47
	3.56

	
	
	
	
	19
	3758
	2.51
	0.01
	0.61
	1.44
	1.71
	1.98
	2.46
	3.06
	3.41
	3.55

	
	
	
	
	20
	3433
	1.61
	0.00
	0.26
	1.26
	1.35
	1.43
	1.55
	1.68
	2.02
	2.67

	
	
	
	
	21
	3377
	1.34
	0.00
	0.18
	0.79
	1.21
	1.25
	1.33
	1.49
	1.53
	1.81

	
	
	
	
	22
	2935
	1.24
	0.00
	0.24
	0.62
	0.71
	1.17
	1.27
	1.39
	1.52
	1.55

	
	
	
	
	23
	3042
	1.30
	0.00
	0.27
	0.72
	0.78
	1.13
	1.34
	1.55
	1.63
	1.71

	
	
	
	
	24
	2815
	1.95
	0.01
	0.39
	0.78
	1.51
	1.71
	1.92
	2.19
	2.51
	3.12

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site B
	36 mesh
	one
	13874
	1
	2951
	3.22
	0.02
	1.07
	0.49
	1.02
	2.81
	3.46
	4.03
	4.38
	4.56

	
	
	
	
	2
	3122
	2.52
	0.02
	0.89
	1.06
	1.60
	1.78
	2.25
	3.17
	4.04
	4.43

	
	
	
	
	3
	2534
	2.07
	0.01
	0.32
	1.51
	1.59
	1.70
	2.15
	2.31
	2.47
	2.68

	
	
	
	
	4
	2264
	2.01
	0.01
	0.32
	1.44
	1.56
	1.66
	2.05
	2.24
	2.40
	2.69

	
	
	
	
	5
	2174
	2.35
	0.01
	0.44
	1.61
	1.82
	2.07
	2.29
	2.52
	3.00
	4.37

	
	
	
	
	6
	1896
	3.85
	0.01
	0.62
	2.39
	2.91
	3.24
	4.08
	4.38
	4.42
	4.46

	
	
	
	
	7
	2985
	3.10
	0.01
	0.66
	2.07
	2.32
	2.54
	2.98
	3.67
	4.09
	4.44

	
	
	
	
	8
	3377
	2.10
	0.00
	0.26
	1.40
	1.85
	1.99
	2.08
	2.24
	2.47
	2.95

	
	
	
	
	9
	3253
	1.70
	0.01
	0.36
	0.90
	1.00
	1.42
	1.83
	1.98
	2.03
	2.47

	
	
	
	
	10
	3432
	1.68
	0.01
	0.31
	1.02
	1.21
	1.48
	1.65
	1.91
	2.08
	2.29

	
	
	
	
	11
	3389
	1.83
	0.01
	0.29
	1.25
	1.48
	1.63
	1.83
	1.99
	2.20
	2.68

	
	
	
	
	12
	3615
	2.33
	0.01
	0.72
	1.09
	1.37
	1.57
	2.42
	2.87
	3.18
	4.47

	
	
	
	
	13
	4244
	3.02
	0.01
	0.90
	1.17
	1.79
	2.32
	3.01
	3.86
	4.26
	4.59

	
	
	
	
	14
	4979
	2.12
	0.01
	0.36
	1.34
	1.65
	1.85
	2.10
	2.40
	2.61
	3.14

	
	
	
	
	15
	4975
	1.91
	0.00
	0.24
	1.35
	1.68
	1.78
	1.94
	2.02
	2.30
	2.71

	
	
	
	
	16
	4854
	1.83
	0.00
	0.23
	1.28
	1.60
	1.69
	1.83
	1.99
	2.14
	2.59

	
	
	
	
	17
	4773
	2.16
	0.01
	0.42
	1.33
	1.74
	1.91
	2.06
	2.29
	2.67
	3.87

	
	
	
	
	18
	3954
	3.82
	0.01
	0.66
	1.91
	2.62
	3.59
	4.09
	4.32
	4.38
	4.48

	
	
	
	
	19
	4492
	3.41
	0.01
	0.71
	2.10
	2.38
	2.73
	3.54
	4.00
	4.33
	4.42

	
	
	
	
	20
	3984
	2.27
	0.01
	0.42
	1.73
	1.87
	1.97
	2.15
	2.47
	2.91
	3.71

	
	
	
	
	21
	3343
	1.82
	0.01
	0.33
	0.73
	1.40
	1.71
	1.88
	2.02
	2.18
	2.47

	
	
	
	
	22
	2925
	1.78
	0.00
	0.25
	1.34
	1.42
	1.48
	1.90
	1.99
	2.04
	2.11

	
	
	
	
	23
	2935
	1.98
	0.00
	0.20
	1.48
	1.61
	1.88
	2.05
	2.12
	2.18
	2.34

	
	
	
	
	24
	2890
	2.73
	0.01
	0.37
	1.90
	2.28
	2.41
	2.76
	3.00
	3.30
	3.55
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	Percentiles

	Site
	Mesh
	Position
	TDR
	Tidal hour
	Count
	Mean
	SE
	SD
	Min
	10%
	25%
	Median
	75%
	90%
	Max

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	1/4 depth
	13901
	1
	1601
	0.94
	0.00
	0.18
	0.56
	0.66
	0.83
	0.93
	1.06
	1.15
	1.34

	
	
	
	
	2
	1778
	0.61
	0.00
	0.18
	0.17
	0.41
	0.48
	0.60
	0.77
	0.85
	1.03

	
	
	
	
	3
	1831
	0.31
	0.00
	0.07
	0.17
	0.19
	0.23
	0.32
	0.35
	0.39
	0.48

	
	
	
	
	4
	1831
	0.31
	0.00
	0.07
	0.18
	0.20
	0.26
	0.33
	0.35
	0.39
	0.42

	
	
	
	
	5
	1831
	0.33
	0.00
	0.07
	0.19
	0.23
	0.28
	0.33
	0.37
	0.43
	0.49

	
	
	
	
	6
	1716
	0.44
	0.00
	0.09
	0.23
	0.33
	0.36
	0.42
	0.52
	0.55
	0.65

	
	
	
	
	7
	1758
	0.73
	0.00
	0.15
	0.46
	0.56
	0.62
	0.70
	0.84
	0.94
	1.18

	
	
	
	
	8
	1079
	1.03
	0.01
	0.27
	0.54
	0.67
	0.81
	1.02
	1.29
	1.43
	1.48

	
	
	
	
	9
	423
	0.41
	0.01
	0.11
	0.22
	0.26
	0.28
	0.45
	0.49
	0.54
	0.59

	
	
	
	
	10
	389
	0.20
	0.00
	0.06
	0.11
	0.14
	0.16
	0.18
	0.23
	0.29
	0.37

	
	
	
	
	11
	421
	0.35
	0.00
	0.10
	0.17
	0.22
	0.28
	0.37
	0.41
	0.48
	0.62

	
	
	
	
	12
	778
	0.64
	0.01
	0.20
	0.29
	0.32
	0.52
	0.69
	0.81
	0.87
	0.95

	
	
	
	
	13
	1416
	1.04
	0.01
	0.25
	0.37
	0.68
	0.89
	1.02
	1.24
	1.38
	1.58

	
	
	
	
	14
	2053
	0.66
	0.01
	0.35
	0.17
	0.26
	0.42
	0.59
	0.87
	0.99
	2.22

	
	
	
	
	15
	2085
	0.34
	0.00
	0.12
	0.15
	0.18
	0.26
	0.34
	0.39
	0.55
	0.69

	
	
	
	
	16
	2114
	0.35
	0.00
	0.10
	0.17
	0.20
	0.31
	0.36
	0.41
	0.51
	0.53

	
	
	
	
	17
	2114
	0.37
	0.00
	0.10
	0.17
	0.21
	0.33
	0.36
	0.41
	0.53
	0.60

	
	
	
	
	18
	2138
	0.45
	0.00
	0.12
	0.21
	0.26
	0.39
	0.44
	0.54
	0.62
	0.73

	
	
	
	
	19
	2130
	0.71
	0.00
	0.20
	0.36
	0.46
	0.55
	0.72
	0.83
	0.93
	1.38

	
	
	
	
	20
	2081
	1.07
	0.01
	0.29
	0.10
	0.76
	0.88
	0.99
	1.27
	1.44
	2.42

	
	
	
	
	21
	1709
	0.61
	0.00
	0.20
	0.24
	0.32
	0.48
	0.58
	0.76
	0.89
	1.00

	
	
	
	
	22
	1945
	0.40
	0.00
	0.17
	0.19
	0.24
	0.29
	0.35
	0.44
	0.71
	0.75

	
	
	
	
	23
	2008
	0.45
	0.01
	0.26
	0.21
	0.23
	0.27
	0.37
	0.50
	0.90
	1.22

	
	
	
	
	24
	1951
	0.65
	0.00
	0.22
	0.32
	0.44
	0.48
	0.56
	0.79
	0.97
	1.27

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	1/2 depth
	13902
	1
	1603
	1.73
	0.01
	0.25
	1.17
	1.36
	1.56
	1.76
	1.91
	2.02
	2.25

	
	
	
	
	2
	1776
	1.26
	0.01
	0.28
	0.69
	0.92
	1.04
	1.28
	1.49
	1.63
	1.89

	
	
	
	
	3
	1831
	0.73
	0.00
	0.10
	0.53
	0.57
	0.66
	0.73
	0.79
	0.86
	0.98

	
	
	
	
	4
	1831
	0.75
	0.00
	0.09
	0.54
	0.59
	0.71
	0.75
	0.80
	0.88
	0.94

	
	
	
	
	5
	1831
	0.80
	0.00
	0.10
	0.61
	0.67
	0.74
	0.78
	0.86
	0.96
	1.08

	
	
	
	
	6
	1718
	1.02
	0.00
	0.15
	0.71
	0.82
	0.89
	1.04
	1.13
	1.19
	1.35

	
	
	
	
	7
	1757
	1.48
	0.00
	0.19
	1.15
	1.25
	1.34
	1.44
	1.62
	1.75
	2.10

	
	
	
	
	8
	1080
	1.86
	0.01
	0.33
	1.18
	1.39
	1.59
	1.87
	2.18
	2.33
	2.39

	
	
	
	
	9
	423
	0.94
	0.01
	0.20
	0.64
	0.67
	0.70
	1.00
	1.11
	1.17
	1.28

	
	
	
	
	10
	389
	0.52
	0.01
	0.10
	0.39
	0.42
	0.44
	0.49
	0.59
	0.71
	0.78

	
	
	
	
	11
	421
	0.89
	0.01
	0.14
	0.60
	0.66
	0.77
	0.94
	0.99
	1.04
	1.19

	
	
	
	
	12
	778
	1.31
	0.01
	0.28
	0.84
	0.90
	1.07
	1.34
	1.57
	1.66
	1.76

	
	
	
	
	13
	1415
	1.84
	0.01
	0.34
	0.97
	1.35
	1.65
	1.85
	2.12
	2.27
	2.44

	
	
	
	
	14
	2053
	1.24
	0.01
	0.46
	0.33
	0.51
	0.95
	1.27
	1.54
	1.76
	2.69

	
	
	
	
	15
	2085
	0.80
	0.01
	0.26
	0.29
	0.33
	0.78
	0.84
	0.89
	1.18
	1.33

	
	
	
	
	16
	2114
	0.84
	0.01
	0.24
	0.31
	0.35
	0.82
	0.89
	0.97
	1.11
	1.15

	
	
	
	
	17
	2114
	0.87
	0.01
	0.26
	0.32
	0.35
	0.82
	0.93
	1.02
	1.17
	1.27

	
	
	
	
	18
	2136
	1.03
	0.01
	0.28
	0.34
	0.41
	1.00
	1.06
	1.22
	1.31
	1.49

	
	
	
	
	19
	2130
	1.48
	0.01
	0.26
	1.00
	1.14
	1.28
	1.49
	1.64
	1.75
	2.25

	
	
	
	
	20
	2081
	1.90
	0.01
	0.36
	0.28
	1.50
	1.70
	1.83
	2.15
	2.32
	3.28

	
	
	
	
	21
	1708
	1.29
	0.01
	0.31
	0.42
	0.87
	1.09
	1.26
	1.52
	1.72
	1.81

	
	
	
	
	22
	1945
	0.89
	0.01
	0.32
	0.42
	0.44
	0.76
	0.83
	1.06
	1.41
	1.48

	
	
	
	
	23
	2009
	0.93
	0.01
	0.38
	0.43
	0.46
	0.73
	0.87
	1.01
	1.59
	1.85

	
	
	
	
	24
	1952
	1.21
	0.01
	0.35
	0.60
	0.80
	0.97
	1.12
	1.48
	1.78
	1.91

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	3/4 depth
	13903
	1
	1601
	2.48
	0.01
	0.48
	1.43
	1.65
	2.19
	2.60
	2.85
	3.00
	3.21

	
	
	
	
	2
	1778
	1.58
	0.01
	0.45
	0.83
	1.05
	1.21
	1.52
	1.91
	2.19
	2.86

	
	
	
	
	3
	1831
	0.84
	0.00
	0.10
	0.63
	0.68
	0.78
	0.83
	0.91
	0.98
	1.12

	
	
	
	
	4
	1831
	0.86
	0.00
	0.10
	0.62
	0.69
	0.81
	0.87
	0.94
	1.00
	1.07

	
	
	
	
	5
	1831
	0.93
	0.00
	0.12
	0.72
	0.79
	0.84
	0.92
	1.01
	1.11
	1.22

	
	
	
	
	6
	1716
	1.21
	0.00
	0.19
	0.85
	0.93
	1.05
	1.25
	1.33
	1.44
	1.65

	
	
	
	
	7
	1758
	1.93
	0.01
	0.38
	1.42
	1.53
	1.64
	1.80
	2.18
	2.52
	3.04

	
	
	
	
	8
	1079
	2.60
	0.02
	0.61
	1.36
	1.65
	2.02
	2.82
	3.14
	3.32
	3.37

	
	
	
	
	9
	423
	1.10
	0.01
	0.23
	0.76
	0.81
	0.83
	1.17
	1.31
	1.38
	1.51

	
	
	
	
	10
	389
	0.61
	0.01
	0.13
	0.46
	0.49
	0.51
	0.56
	0.70
	0.85
	0.91

	
	
	
	
	11
	421
	1.13
	0.01
	0.17
	0.76
	0.83
	1.03
	1.20
	1.24
	1.28
	1.44

	
	
	
	
	12
	778
	1.68
	0.01
	0.40
	1.14
	1.23
	1.29
	1.60
	2.04
	2.25
	2.48

	
	
	
	
	13
	1416
	2.65
	0.01
	0.52
	1.42
	1.72
	2.35
	2.72
	3.09
	3.25
	3.45

	
	
	
	
	14
	2053
	1.56
	0.01
	0.58
	0.45
	0.78
	1.14
	1.53
	1.97
	2.37
	3.03

	
	
	
	
	15
	2085
	0.93
	0.01
	0.27
	0.40
	0.44
	0.88
	0.95
	1.03
	1.33
	1.57

	
	
	
	
	16
	2114
	0.98
	0.01
	0.26
	0.45
	0.47
	0.93
	1.03
	1.15
	1.27
	1.31

	
	
	
	
	17
	2114
	1.02
	0.01
	0.28
	0.46
	0.49
	0.94
	1.06
	1.23
	1.36
	1.49

	
	
	
	
	18
	2138
	1.24
	0.01
	0.32
	0.49
	0.56
	1.15
	1.26
	1.46
	1.58
	1.83

	
	
	
	
	19
	2130
	1.92
	0.01
	0.46
	1.20
	1.34
	1.57
	1.87
	2.17
	2.50
	3.23

	
	
	
	
	20
	2081
	2.68
	0.01
	0.57
	0.85
	1.82
	2.30
	2.71
	3.14
	3.31
	4.33

	
	
	
	
	21
	1709
	1.57
	0.01
	0.48
	0.38
	1.01
	1.24
	1.48
	1.88
	2.28
	2.62

	
	
	
	
	22
	1945
	1.01
	0.01
	0.43
	0.37
	0.40
	0.86
	0.93
	1.24
	1.72
	1.80

	
	
	
	
	23
	2008
	1.05
	0.01
	0.45
	0.40
	0.43
	0.82
	1.02
	1.18
	1.80
	2.03

	
	
	
	
	24
	1951
	1.44
	0.01
	0.52
	0.53
	0.71
	1.13
	1.32
	1.85
	2.27
	2.71

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	45 mesh
	1/4 depth
	13880
	1
	1123
	0.78
	0.01
	0.32
	0.14
	0.26
	0.56
	0.78
	1.06
	1.14
	1.33

	
	
	
	
	2
	1213
	0.30
	0.01
	0.25
	0.00
	0.07
	0.13
	0.23
	0.38
	0.70
	1.28

	
	
	
	
	3
	1486
	0.07
	0.00
	0.04
	0.00
	0.03
	0.05
	0.07
	0.10
	0.12
	0.19

	
	
	
	
	4
	1486
	0.07
	0.00
	0.03
	0.02
	0.04
	0.05
	0.07
	0.09
	0.12
	0.15

	
	
	
	
	5
	1486
	0.07
	0.00
	0.04
	0.00
	0.03
	0.05
	0.06
	0.09
	0.14
	0.18

	
	
	
	
	6
	1301
	0.10
	0.00
	0.07
	0.00
	0.03
	0.05
	0.09
	0.13
	0.21
	0.30

	
	
	
	
	7
	939
	0.17
	0.00
	0.13
	0.02
	0.05
	0.08
	0.13
	0.22
	0.31
	0.84

	
	
	
	
	8
	576
	0.79
	0.01
	0.33
	0.21
	0.28
	0.49
	0.88
	1.08
	1.15
	1.21

	
	
	
	
	9
	389
	0.12
	0.00
	0.05
	0.02
	0.06
	0.07
	0.13
	0.16
	0.18
	0.21

	
	
	
	
	10
	389
	0.21
	0.01
	0.14
	0.04
	0.06
	0.09
	0.14
	0.35
	0.41
	0.47

	
	
	
	
	11
	389
	0.30
	0.01
	0.15
	0.10
	0.14
	0.17
	0.25
	0.39
	0.51
	0.69

	
	
	
	
	12
	322
	0.48
	0.01
	0.18
	0.08
	0.34
	0.36
	0.43
	0.63
	0.73
	0.85

	
	
	
	
	13
	973
	0.79
	0.01
	0.25
	0.16
	0.46
	0.63
	0.76
	0.98
	1.15
	1.46

	
	
	
	
	14
	1878
	0.25
	0.00
	0.14
	0.05
	0.09
	0.14
	0.22
	0.32
	0.46
	0.78

	
	
	
	
	15
	2114
	0.12
	0.00
	0.06
	0.02
	0.06
	0.07
	0.10
	0.14
	0.22
	0.27

	
	
	
	
	16
	2114
	0.11
	0.00
	0.06
	0.03
	0.04
	0.06
	0.09
	0.12
	0.23
	0.26

	
	
	
	
	17
	2114
	0.11
	0.00
	0.07
	0.03
	0.05
	0.06
	0.09
	0.12
	0.25
	0.32

	
	
	
	
	18
	1963
	0.14
	0.00
	0.09
	0.02
	0.05
	0.07
	0.12
	0.16
	0.30
	0.41

	
	
	
	
	19
	2072
	0.26
	0.00
	0.16
	0.07
	0.10
	0.17
	0.22
	0.27
	0.41
	0.84

	
	
	
	
	20
	1848
	0.84
	0.01
	0.39
	0.17
	0.29
	0.55
	0.83
	1.16
	1.36
	1.64

	
	
	
	
	21
	1542
	0.31
	0.00
	0.16
	0.04
	0.08
	0.18
	0.29
	0.41
	0.55
	0.77

	
	
	
	
	22
	1868
	0.17
	0.00
	0.11
	0.02
	0.07
	0.09
	0.14
	0.20
	0.32
	0.50

	
	
	
	
	23
	1904
	0.34
	0.01
	0.41
	0.04
	0.08
	0.13
	0.19
	0.35
	0.50
	1.73

	
	
	
	
	24
	1954
	0.37
	0.01
	0.35
	0.06
	0.10
	0.12
	0.31
	0.40
	0.66
	1.84

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	45 mesh
	1/2 depth
	13883
	1
	1118
	1.77
	0.02
	0.60
	0.33
	0.56
	1.53
	1.95
	2.26
	2.34
	2.56

	
	
	
	
	2
	1319
	0.83
	0.02
	0.58
	0.08
	0.20
	0.35
	0.68
	1.22
	1.73
	2.54

	
	
	
	
	3
	1831
	0.17
	0.00
	0.13
	-0.01
	0.01
	0.04
	0.15
	0.30
	0.37
	0.47

	
	
	
	
	4
	1831
	0.16
	0.00
	0.15
	0.00
	0.01
	0.02
	0.14
	0.23
	0.41
	0.47

	
	
	
	
	5
	1831
	0.19
	0.00
	0.17
	-0.01
	0.01
	0.02
	0.16
	0.31
	0.45
	0.51

	
	
	
	
	6
	1665
	0.30
	0.01
	0.26
	-0.02
	0.01
	0.04
	0.23
	0.49
	0.61
	0.92

	
	
	
	
	7
	1147
	0.82
	0.01
	0.43
	0.00
	0.18
	0.54
	0.84
	1.10
	1.35
	2.09

	
	
	
	
	8
	575
	1.87
	0.02
	0.56
	0.66
	0.95
	1.43
	2.10
	2.35
	2.42
	2.47

	
	
	
	
	9
	389
	0.36
	0.01
	0.13
	0.17
	0.19
	0.23
	0.35
	0.43
	0.55
	0.65

	
	
	
	
	10
	389
	0.29
	0.01
	0.14
	0.11
	0.14
	0.16
	0.24
	0.45
	0.51
	0.56

	
	
	
	
	11
	451
	0.56
	0.01
	0.13
	0.33
	0.37
	0.49
	0.55
	0.64
	0.73
	0.96

	
	
	
	
	12
	718
	0.92
	0.01
	0.32
	0.46
	0.61
	0.66
	0.78
	1.23
	1.40
	1.94

	
	
	
	
	13
	1054
	1.59
	0.02
	0.51
	0.64
	0.91
	1.20
	1.57
	1.98
	2.40
	2.76

	
	
	
	
	14
	1876
	0.63
	0.01
	0.44
	0.09
	0.13
	0.27
	0.48
	0.95
	1.34
	1.75

	
	
	
	
	15
	2114
	0.29
	0.00
	0.22
	0.04
	0.09
	0.11
	0.25
	0.32
	0.73
	0.89

	
	
	
	
	16
	2114
	0.27
	0.00
	0.22
	0.02
	0.04
	0.09
	0.22
	0.32
	0.70
	0.75

	
	
	
	
	17
	2114
	0.32
	0.01
	0.23
	0.02
	0.06
	0.08
	0.30
	0.44
	0.74
	0.80

	
	
	
	
	18
	1959
	0.43
	0.01
	0.31
	0.06
	0.09
	0.12
	0.39
	0.55
	0.98
	1.31

	
	
	
	
	19
	2069
	0.86
	0.01
	0.58
	0.09
	0.18
	0.27
	0.88
	1.37
	1.57
	2.16

	
	
	
	
	20
	1845
	1.90
	0.02
	0.71
	0.28
	0.62
	1.55
	2.08
	2.46
	2.65
	2.88

	
	
	
	
	21
	1542
	0.85
	0.01
	0.30
	0.35
	0.46
	0.62
	0.80
	1.02
	1.31
	1.96

	
	
	
	
	22
	1868
	0.42
	0.00
	0.16
	0.14
	0.19
	0.34
	0.39
	0.51
	0.66
	0.74

	
	
	
	
	23
	1901
	0.66
	0.01
	0.47
	0.14
	0.22
	0.32
	0.53
	0.83
	1.30
	1.99

	
	
	
	
	24
	1950
	1.02
	0.01
	0.50
	0.18
	0.22
	0.85
	1.03
	1.27
	1.64
	2.14

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	45 mesh
	3/4 depth
	13885
	1
	1118
	2.78
	0.02
	0.77
	1.06
	1.47
	2.32
	2.71
	3.38
	3.68
	4.06

	
	
	
	
	2
	1319
	1.31
	0.02
	0.56
	0.57
	0.77
	0.87
	1.15
	1.68
	2.09
	3.98

	
	
	
	
	3
	1831
	0.56
	0.00
	0.13
	0.25
	0.32
	0.50
	0.59
	0.64
	0.72
	0.84

	
	
	
	
	4
	1831
	0.55
	0.00
	0.12
	0.26
	0.34
	0.50
	0.58
	0.65
	0.67
	0.70

	
	
	
	
	5
	1831
	0.63
	0.00
	0.14
	0.31
	0.41
	0.55
	0.67
	0.73
	0.78
	0.90

	
	
	
	
	6
	1665
	0.90
	0.01
	0.27
	0.42
	0.53
	0.70
	0.89
	1.10
	1.29
	1.39

	
	
	
	
	7
	1147
	1.79
	0.02
	0.63
	0.65
	1.09
	1.38
	1.59
	2.18
	2.77
	3.63

	
	
	
	
	8
	575
	3.19
	0.03
	0.72
	1.59
	2.03
	2.58
	3.51
	3.81
	3.89
	3.97

	
	
	
	
	9
	389
	1.08
	0.01
	0.27
	0.67
	0.72
	0.78
	1.12
	1.28
	1.47
	1.59

	
	
	
	
	10
	389
	0.77
	0.01
	0.23
	0.44
	0.49
	0.55
	0.78
	1.03
	1.07
	1.13

	
	
	
	
	11
	451
	1.32
	0.01
	0.28
	0.73
	0.76
	1.09
	1.44
	1.49
	1.57
	1.76

	
	
	
	
	12
	718
	1.34
	0.02
	0.59
	0.77
	0.80
	0.87
	0.98
	1.78
	2.21
	3.18

	
	
	
	
	13
	1054
	2.19
	0.03
	1.08
	0.63
	1.00
	1.16
	2.02
	3.16
	3.82
	4.25

	
	
	
	
	14
	1876
	1.09
	0.01
	0.55
	0.27
	0.37
	0.73
	1.02
	1.32
	1.96
	2.70

	
	
	
	
	15
	2114
	0.66
	0.01
	0.23
	0.22
	0.26
	0.51
	0.71
	0.84
	0.93
	1.11

	
	
	
	
	16
	2114
	0.64
	0.00
	0.21
	0.22
	0.27
	0.58
	0.61
	0.78
	0.83
	1.10

	
	
	
	
	17
	2114
	0.74
	0.01
	0.27
	0.26
	0.32
	0.61
	0.69
	0.90
	1.15
	1.27

	
	
	
	
	18
	1959
	0.94
	0.01
	0.39
	0.22
	0.32
	0.70
	0.97
	1.25
	1.40
	1.67

	
	
	
	
	19
	2069
	1.80
	0.01
	0.68
	0.32
	1.03
	1.09
	1.84
	2.46
	2.75
	3.18

	
	
	
	
	20
	1845
	2.98
	0.02
	0.96
	0.81
	1.51
	2.28
	3.14
	3.85
	4.08
	4.34

	
	
	
	
	21
	1542
	1.33
	0.02
	0.62
	0.31
	0.49
	0.86
	1.36
	1.76
	2.15
	3.11

	
	
	
	
	22
	1868
	0.81
	0.01
	0.30
	0.31
	0.35
	0.58
	0.77
	1.03
	1.22
	1.48

	
	
	
	
	23
	1901
	1.04
	0.01
	0.44
	0.43
	0.67
	0.76
	0.93
	1.10
	1.82
	3.01

	
	
	
	
	24
	1950
	1.55
	0.01
	0.53
	0.69
	0.74
	1.20
	1.62
	1.96
	2.16
	3.06

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 





[bookmark: _Toc459796176]Leadline depths (m) summarized by site
	 
	 
	 
	 
	Leadline Depth Distribution (m)

	
	
	
	
	
	
	
	Percentiles

	Site
	Mesh
	Tidal hour
	Count
	Mean
	SE
	SD
	Min
	10%
	25%
	Median
	75%
	90%
	Max

	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	29 mesh
	1
	4142
	3.13
	0.01
	0.59
	1.42
	2.37
	2.76
	3.27
	3.67
	3.74
	3.88

	
	
	2
	4668
	2.26
	0.01
	0.69
	0.90
	1.25
	1.84
	2.27
	2.69
	3.25
	3.73

	
	
	3
	5349
	1.44
	0.01
	0.49
	0.65
	0.74
	0.86
	1.67
	1.83
	1.97
	2.46

	
	
	4
	5465
	1.41
	0.01
	0.46
	0.67
	0.77
	0.93
	1.55
	1.78
	1.93
	2.16

	
	
	5
	5465
	1.50
	0.01
	0.47
	0.74
	0.83
	1.01
	1.66
	1.91
	2.06
	2.32

	
	
	6
	5050
	1.84
	0.01
	0.56
	0.84
	1.14
	1.35
	1.88
	2.31
	2.63
	3.07

	
	
	7
	4968
	2.60
	0.01
	0.61
	1.45
	1.72
	2.04
	2.70
	3.09
	3.33
	3.79

	
	
	8
	2852
	3.21
	0.01
	0.63
	1.43
	2.19
	2.85
	3.39
	3.74
	3.77
	4.01

	
	
	9
	1494
	1.76
	0.01
	0.54
	0.77
	0.95
	1.41
	1.75
	1.99
	2.54
	2.97

	
	
	10
	1586
	1.40
	0.01
	0.55
	0.44
	0.54
	0.96
	1.55
	1.94
	2.02
	2.33

	
	
	11
	1879
	2.04
	0.01
	0.61
	0.74
	1.22
	1.71
	2.07
	2.51
	2.80
	3.48

	
	
	12
	2965
	2.61
	0.01
	0.67
	1.18
	1.45
	1.93
	2.83
	3.12
	3.30
	3.68

	
	
	13
	4768
	3.25
	0.01
	0.58
	1.22
	2.45
	3.00
	3.34
	3.72
	3.78
	4.10

	
	
	14
	7374
	2.36
	0.01
	0.76
	0.51
	1.23
	1.92
	2.38
	2.84
	3.19
	4.99

	
	
	15
	7658
	1.60
	0.01
	0.52
	0.43
	0.89
	1.33
	1.66
	1.99
	2.23
	2.73

	
	
	16
	7416
	1.69
	0.01
	0.64
	0.51
	0.93
	1.24
	1.65
	2.08
	2.55
	3.71

	
	
	17
	7716
	1.79
	0.01
	0.70
	0.55
	0.97
	1.26
	1.75
	2.18
	2.70
	3.92

	
	
	18
	7508
	1.87
	0.01
	0.58
	0.58
	1.16
	1.48
	1.77
	2.27
	2.67
	3.71

	
	
	19
	7644
	2.58
	0.01
	0.62
	1.13
	1.77
	2.16
	2.57
	3.06
	3.33
	3.83

	
	
	20
	7201
	3.25
	0.01
	0.51
	1.19
	2.64
	2.95
	3.29
	3.71
	3.80
	4.98

	
	
	21
	5999
	2.49
	0.01
	0.71
	0.34
	1.39
	1.95
	2.63
	3.03
	3.33
	3.76

	
	
	22
	6410
	1.87
	0.01
	0.68
	0.33
	0.92
	1.55
	2.06
	2.42
	2.63
	3.00

	
	
	23
	5231
	1.81
	0.01
	0.71
	0.37
	0.85
	1.14
	1.98
	2.35
	2.63
	3.02

	
	
	24
	5164
	2.30
	0.01
	0.77
	0.49
	1.18
	1.61
	2.49
	2.85
	3.13
	3.70

	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site A
	45 mesh
	1
	4044
	4.71
	0.02
	1.15
	1.79
	2.95
	3.85
	5.10
	5.58
	5.76
	7.19

	
	
	2
	4334
	3.00
	0.02
	1.47
	0.59
	0.90
	1.85
	2.98
	4.14
	5.07
	6.07

	
	
	3
	5493
	1.40
	0.01
	0.72
	0.32
	0.54
	0.63
	1.59
	1.99
	2.35
	3.08

	
	
	4
	5493
	1.39
	0.01
	0.69
	0.35
	0.54
	0.64
	1.64
	1.93
	2.15
	2.68

	
	
	5
	5433
	1.59
	0.01
	0.79
	0.37
	0.60
	0.71
	1.85
	2.20
	2.59
	3.47

	
	
	6
	4966
	2.20
	0.02
	1.11
	0.45
	0.70
	1.04
	2.48
	3.17
	3.56
	4.21

	
	
	7
	3714
	3.67
	0.02
	1.36
	0.74
	1.67
	2.49
	3.89
	4.94
	5.26
	5.74

	
	
	8
	1843
	4.90
	0.02
	0.99
	1.74
	3.36
	4.62
	5.18
	5.57
	5.78
	6.33

	
	
	9
	1167
	2.27
	0.03
	1.02
	0.68
	0.84
	1.32
	2.47
	2.95
	3.67
	4.49

	
	
	10
	1167
	1.74
	0.03
	0.92
	0.45
	0.56
	1.01
	1.85
	2.41
	2.91
	3.80

	
	
	11
	1227
	2.69
	0.03
	1.08
	0.77
	1.26
	1.54
	3.31
	3.62
	3.86
	4.00

	
	
	12
	1903
	2.82
	0.03
	1.30
	0.80
	0.95
	1.48
	3.14
	4.00
	4.26
	5.27

	
	
	13
	2825
	4.23
	0.03
	1.47
	0.74
	1.60
	3.45
	4.91
	5.21
	5.48
	6.35

	
	
	14
	5621
	2.84
	0.02
	1.36
	0.24
	1.03
	1.48
	3.04
	3.91
	4.53
	5.56

	
	
	15
	6342
	1.64
	0.01
	0.78
	0.18
	0.61
	0.84
	1.78
	2.21
	2.58
	3.47

	
	
	16
	6342
	1.54
	0.01
	0.69
	0.20
	0.63
	0.77
	1.69
	2.04
	2.23
	3.06

	
	
	17
	6342
	1.75
	0.01
	0.78
	0.23
	0.71
	0.91
	2.00
	2.29
	2.62
	3.45

	
	
	18
	6038
	2.24
	0.01
	0.97
	0.26
	0.88
	1.29
	2.46
	3.00
	3.44
	3.94

	
	
	19
	5985
	3.47
	0.02
	1.26
	0.38
	1.37
	2.54
	3.77
	4.45
	4.94
	5.68

	
	
	20
	5624
	4.80
	0.02
	1.16
	0.57
	3.14
	4.52
	5.24
	5.45
	5.78
	6.31

	
	
	21
	4282
	2.98
	0.02
	1.47
	0.22
	0.92
	1.76
	3.27
	4.12
	4.75
	5.84

	
	
	22
	5294
	1.98
	0.01
	1.07
	0.22
	0.60
	1.12
	1.86
	2.98
	3.51
	3.81

	
	
	23
	5444
	2.20
	0.01
	1.01
	0.34
	0.78
	1.19
	2.27
	2.97
	3.57
	4.49

	
	
	24
	5757
	3.10
	0.02
	1.34
	1.00
	1.45
	1.84
	2.93
	4.16
	4.85
	7.00

	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site B
	29 mesh
	1
	6571
	2.64
	0.01
	0.96
	0.00
	1.04
	2.35
	2.95
	3.34
	3.48
	3.73

	
	
	2
	6659
	1.80
	0.01
	0.59
	0.28
	1.11
	1.39
	1.75
	2.14
	2.55
	3.52

	
	
	3
	6734
	1.55
	0.00
	0.32
	0.84
	1.13
	1.33
	1.55
	1.80
	1.98
	2.13

	
	
	4
	7201
	1.52
	0.00
	0.33
	0.82
	1.08
	1.32
	1.41
	1.77
	1.99
	2.16

	
	
	5
	7008
	1.75
	0.01
	0.43
	0.94
	1.35
	1.44
	1.66
	2.04
	2.30
	3.12

	
	
	6
	6004
	2.76
	0.01
	0.59
	0.68
	1.93
	2.29
	2.84
	3.27
	3.43
	3.61

	
	
	7
	6748
	2.71
	0.01
	0.60
	1.32
	1.81
	2.25
	2.78
	3.29
	3.40
	3.60

	
	
	8
	6550
	1.69
	0.00
	0.37
	1.17
	1.28
	1.39
	1.61
	1.93
	2.18
	2.96

	
	
	9
	5805
	1.47
	0.00
	0.33
	0.73
	1.12
	1.19
	1.38
	1.80
	1.86
	2.19

	
	
	10
	5890
	1.49
	0.00
	0.35
	0.47
	1.12
	1.22
	1.37
	1.78
	1.97
	2.45

	
	
	11
	5833
	1.57
	0.01
	0.52
	-0.02
	1.22
	1.38
	1.53
	1.88
	2.13
	2.68

	
	
	12
	6026
	2.04
	0.01
	0.64
	-0.12
	0.97
	1.65
	2.11
	2.49
	2.79
	3.39

	
	
	13
	6351
	2.73
	0.01
	0.71
	0.78
	1.67
	2.30
	2.84
	3.35
	3.48
	3.71

	
	
	14
	6164
	1.77
	0.01
	0.42
	1.14
	1.37
	1.51
	1.65
	1.93
	2.41
	3.37

	
	
	15
	5963
	1.51
	0.00
	0.34
	1.12
	1.24
	1.32
	1.44
	1.59
	1.81
	3.47

	
	
	16
	5992
	1.39
	0.00
	0.19
	1.10
	1.17
	1.25
	1.35
	1.49
	1.69
	1.90

	
	
	17
	6026
	1.58
	0.00
	0.33
	1.11
	1.23
	1.34
	1.52
	1.78
	2.09
	2.60

	
	
	18
	5372
	2.81
	0.01
	0.61
	1.38
	1.85
	2.34
	3.00
	3.37
	3.46
	3.56

	
	
	19
	5322
	2.64
	0.01
	0.62
	1.44
	1.77
	2.09
	2.66
	3.26
	3.43
	3.65

	
	
	20
	4181
	1.64
	0.00
	0.26
	1.26
	1.37
	1.46
	1.58
	1.75
	2.01
	2.67

	
	
	21
	4450
	1.41
	0.00
	0.23
	0.79
	1.22
	1.27
	1.36
	1.53
	1.73
	2.18

	
	
	22
	4713
	1.31
	0.00
	0.27
	0.55
	0.97
	1.19
	1.33
	1.49
	1.54
	2.18

	
	
	23
	5324
	1.37
	0.01
	0.49
	0.01
	0.75
	1.18
	1.46
	1.62
	1.80
	2.52

	
	
	24
	5283
	2.03
	0.01
	0.76
	0.00
	1.31
	1.71
	2.08
	2.58
	2.89
	3.40

	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Site B
	36 mesh
	1
	2951
	3.22
	0.02
	1.07
	0.49
	1.02
	2.81
	3.46
	4.03
	4.38
	4.56

	
	
	2
	3122
	2.52
	0.02
	0.89
	1.06
	1.60
	1.78
	2.25
	3.17
	4.04
	4.43

	
	
	3
	2534
	2.07
	0.01
	0.32
	1.51
	1.59
	1.70
	2.15
	2.31
	2.47
	2.68

	
	
	4
	2264
	2.01
	0.01
	0.32
	1.44
	1.56
	1.66
	2.05
	2.24
	2.40
	2.69

	
	
	5
	2174
	2.35
	0.01
	0.44
	1.61
	1.82
	2.07
	2.29
	2.52
	3.00
	4.37

	
	
	6
	1896
	3.85
	0.01
	0.62
	2.39
	2.91
	3.24
	4.08
	4.38
	4.42
	4.46

	
	
	7
	2985
	3.10
	0.01
	0.66
	2.07
	2.32
	2.54
	2.98
	3.67
	4.09
	4.44

	
	
	8
	3377
	2.10
	0.00
	0.26
	1.40
	1.85
	1.99
	2.08
	2.24
	2.47
	2.95

	
	
	9
	3253
	1.70
	0.01
	0.36
	0.90
	1.00
	1.42
	1.83
	1.98
	2.03
	2.47

	
	
	10
	3432
	1.68
	0.01
	0.31
	1.02
	1.21
	1.48
	1.65
	1.91
	2.08
	2.29

	
	
	11
	3389
	1.83
	0.01
	0.29
	1.25
	1.48
	1.63
	1.83
	1.99
	2.20
	2.68

	
	
	12
	3615
	2.33
	0.01
	0.72
	1.09
	1.37
	1.57
	2.42
	2.87
	3.18
	4.47

	
	
	13
	4244
	3.02
	0.01
	0.90
	1.17
	1.79
	2.32
	3.01
	3.86
	4.26
	4.59

	
	
	14
	4979
	2.12
	0.01
	0.36
	1.34
	1.65
	1.85
	2.10
	2.40
	2.61
	3.14

	
	
	15
	4975
	1.91
	0.00
	0.24
	1.35
	1.68
	1.78
	1.94
	2.02
	2.30
	2.71

	
	
	16
	4854
	1.83
	0.00
	0.23
	1.28
	1.60
	1.69
	1.83
	1.99
	2.14
	2.59

	
	
	17
	4773
	2.16
	0.01
	0.42
	1.33
	1.74
	1.91
	2.06
	2.29
	2.67
	3.87

	
	
	18
	3954
	3.82
	0.01
	0.66
	1.91
	2.62
	3.59
	4.09
	4.32
	4.38
	4.48

	
	
	19
	4492
	3.41
	0.01
	0.71
	2.10
	2.38
	2.73
	3.54
	4.00
	4.33
	4.42

	
	
	20
	3984
	2.27
	0.01
	0.42
	1.73
	1.87
	1.97
	2.15
	2.47
	2.91
	3.71

	
	
	21
	3343
	1.82
	0.01
	0.33
	0.73
	1.40
	1.71
	1.88
	2.02
	2.18
	2.47

	
	
	22
	2925
	1.78
	0.00
	0.25
	1.34
	1.42
	1.48
	1.90
	1.99
	2.04
	2.11

	
	
	23
	2935
	1.98
	0.00
	0.20
	1.48
	1.61
	1.88
	2.05
	2.12
	2.18
	2.34

	
	
	24
	2890
	2.73
	0.01
	0.37
	1.90
	2.28
	2.41
	2.76
	3.00
	3.30
	3.55

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 





[bookmark: _Toc459796177]Leadline depths (m) summarized across all nets
	 
	 
	 
	Leadline Depth Distribution (m)

	
	
	
	
	
	
	Percentiles

	Mesh
	Tidal hour
	Count
	Mean
	SE
	SD
	Min
	10%
	25%
	Median
	75%
	90%
	Max

	
	
	
	
	
	
	
	
	
	
	
	
	

	29 mesh
	1
	10713
	2.83
	0.01
	0.87
	0.00
	1.66
	2.56
	3.08
	3.44
	3.67
	3.88

	
	2
	11327
	1.99
	0.01
	0.67
	0.28
	1.18
	1.48
	1.98
	2.38
	2.93
	3.73

	
	3
	12083
	1.50
	0.00
	0.41
	0.65
	0.85
	1.21
	1.57
	1.81
	1.98
	2.46

	
	4
	12666
	1.47
	0.00
	0.39
	0.67
	0.86
	1.21
	1.48
	1.78
	1.98
	2.16

	
	5
	12473
	1.64
	0.00
	0.47
	0.74
	0.97
	1.37
	1.66
	1.96
	2.19
	3.12

	
	6
	11054
	2.34
	0.01
	0.73
	0.68
	1.32
	1.83
	2.33
	2.96
	3.34
	3.61

	
	7
	11716
	2.67
	0.01
	0.60
	1.32
	1.77
	2.19
	2.74
	3.20
	3.39
	3.79

	
	8
	9402
	2.15
	0.01
	0.84
	1.17
	1.31
	1.46
	1.86
	2.76
	3.71
	4.01

	
	9
	7299
	1.53
	0.00
	0.40
	0.73
	1.12
	1.20
	1.45
	1.82
	1.99
	2.97

	
	10
	7476
	1.47
	0.00
	0.40
	0.44
	1.06
	1.20
	1.39
	1.79
	2.00
	2.45

	
	11
	7712
	1.68
	0.01
	0.58
	-0.02
	1.22
	1.39
	1.63
	2.00
	2.50
	3.48

	
	12
	8991
	2.23
	0.01
	0.70
	-0.12
	1.35
	1.75
	2.29
	2.76
	3.12
	3.68

	
	13
	11119
	2.95
	0.01
	0.71
	0.78
	1.94
	2.55
	3.20
	3.46
	3.72
	4.10

	
	14
	13538
	2.09
	0.01
	0.69
	0.51
	1.33
	1.57
	1.97
	2.57
	3.04
	4.99

	
	15
	13621
	1.56
	0.00
	0.45
	0.43
	0.96
	1.32
	1.52
	1.80
	2.17
	3.47

	
	16
	13408
	1.56
	0.00
	0.51
	0.51
	1.05
	1.25
	1.42
	1.77
	2.20
	3.71

	
	17
	13742
	1.70
	0.00
	0.58
	0.55
	1.11
	1.30
	1.61
	1.98
	2.34
	3.92

	
	18
	12880
	2.26
	0.01
	0.75
	0.58
	1.31
	1.64
	2.22
	2.88
	3.38
	3.71

	
	19
	12966
	2.60
	0.01
	0.62
	1.13
	1.77
	2.12
	2.60
	3.15
	3.42
	3.83

	
	20
	11382
	2.66
	0.01
	0.89
	1.19
	1.47
	1.69
	2.87
	3.39
	3.76
	4.98

	
	21
	10449
	2.03
	0.01
	0.77
	0.34
	1.25
	1.35
	1.75
	2.70
	3.18
	3.76

	
	22
	11123
	1.63
	0.01
	0.61
	0.33
	0.92
	1.21
	1.52
	2.13
	2.54
	3.00

	
	23
	10555
	1.59
	0.01
	0.64
	0.01
	0.77
	1.16
	1.57
	2.08
	2.43
	3.02

	
	24
	10447
	2.16
	0.01
	0.78
	0.00
	1.19
	1.71
	2.34
	2.71
	3.03
	3.70

	
	
	
	
	
	
	
	
	
	
	
	
	

	36 mesh
	1
	2951
	3.22
	0.02
	1.07
	0.49
	1.02
	2.81
	3.46
	4.03
	4.38
	4.56

	
	2
	3122
	2.52
	0.02
	0.89
	1.06
	1.60
	1.78
	2.25
	3.17
	4.04
	4.43

	
	3
	2534
	2.07
	0.01
	0.32
	1.51
	1.59
	1.70
	2.15
	2.31
	2.47
	2.68

	
	4
	2264
	2.01
	0.01
	0.32
	1.44
	1.56
	1.66
	2.05
	2.24
	2.40
	2.69

	
	5
	2174
	2.35
	0.01
	0.44
	1.61
	1.82
	2.07
	2.29
	2.52
	3.00
	4.37

	
	6
	1896
	3.85
	0.01
	0.62
	2.39
	2.91
	3.24
	4.08
	4.38
	4.42
	4.46

	
	7
	2985
	3.10
	0.01
	0.66
	2.07
	2.32
	2.54
	2.98
	3.67
	4.09
	4.44

	
	8
	3377
	2.10
	0.00
	0.26
	1.40
	1.85
	1.99
	2.08
	2.24
	2.47
	2.95

	
	9
	3253
	1.70
	0.01
	0.36
	0.90
	1.00
	1.42
	1.83
	1.98
	2.03
	2.47

	
	10
	3432
	1.68
	0.01
	0.31
	1.02
	1.21
	1.48
	1.65
	1.91
	2.08
	2.29

	
	11
	3389
	1.83
	0.01
	0.29
	1.25
	1.48
	1.63
	1.83
	1.99
	2.20
	2.68

	
	12
	3615
	2.33
	0.01
	0.72
	1.09
	1.37
	1.57
	2.42
	2.87
	3.18
	4.47

	
	13
	4244
	3.02
	0.01
	0.90
	1.17
	1.79
	2.32
	3.01
	3.86
	4.26
	4.59

	
	14
	4979
	2.12
	0.01
	0.36
	1.34
	1.65
	1.85
	2.10
	2.40
	2.61
	3.14

	
	15
	4975
	1.91
	0.00
	0.24
	1.35
	1.68
	1.78
	1.94
	2.02
	2.30
	2.71

	
	16
	4854
	1.83
	0.00
	0.23
	1.28
	1.60
	1.69
	1.83
	1.99
	2.14
	2.59

	
	17
	4773
	2.16
	0.01
	0.42
	1.33
	1.74
	1.91
	2.06
	2.29
	2.67
	3.87

	
	18
	3954
	3.82
	0.01
	0.66
	1.91
	2.62
	3.59
	4.09
	4.32
	4.38
	4.48

	
	19
	4492
	3.41
	0.01
	0.71
	2.10
	2.38
	2.73
	3.54
	4.00
	4.33
	4.42

	
	20
	3984
	2.27
	0.01
	0.42
	1.73
	1.87
	1.97
	2.15
	2.47
	2.91
	3.71

	
	21
	3343
	1.82
	0.01
	0.33
	0.73
	1.40
	1.71
	1.88
	2.02
	2.18
	2.47

	
	22
	2925
	1.78
	0.00
	0.25
	1.34
	1.42
	1.48
	1.90
	1.99
	2.04
	2.11

	
	23
	2935
	1.98
	0.00
	0.20
	1.48
	1.61
	1.88
	2.05
	2.12
	2.18
	2.34

	
	24
	2890
	2.73
	0.01
	0.37
	1.90
	2.28
	2.41
	2.76
	3.00
	3.30
	3.55

	
	
	
	
	
	
	
	
	
	
	
	
	

	45 mesh
	1
	4044
	4.71
	0.02
	1.15
	1.79
	2.95
	3.85
	5.10
	5.58
	5.76
	7.19

	
	2
	4334
	3.00
	0.02
	1.47
	0.59
	0.90
	1.85
	2.98
	4.14
	5.07
	6.07

	
	3
	5493
	1.40
	0.01
	0.72
	0.32
	0.54
	0.63
	1.59
	1.99
	2.35
	3.08

	
	4
	5493
	1.39
	0.01
	0.69
	0.35
	0.54
	0.64
	1.64
	1.93
	2.15
	2.68

	
	5
	5433
	1.59
	0.01
	0.79
	0.37
	0.60
	0.71
	1.85
	2.20
	2.59
	3.47

	
	6
	4966
	2.20
	0.02
	1.11
	0.45
	0.70
	1.04
	2.48
	3.17
	3.56
	4.21

	
	7
	3714
	3.67
	0.02
	1.36
	0.74
	1.67
	2.49
	3.89
	4.94
	5.26
	5.74

	
	8
	1843
	4.90
	0.02
	0.99
	1.74
	3.36
	4.62
	5.18
	5.57
	5.78
	6.33

	
	9
	1167
	2.27
	0.03
	1.02
	0.68
	0.84
	1.32
	2.47
	2.95
	3.67
	4.49

	
	10
	1167
	1.74
	0.03
	0.92
	0.45
	0.56
	1.01
	1.85
	2.41
	2.91
	3.80

	
	11
	1227
	2.69
	0.03
	1.08
	0.77
	1.26
	1.54
	3.31
	3.62
	3.86
	4.00

	
	12
	1903
	2.82
	0.03
	1.30
	0.80
	0.95
	1.48
	3.14
	4.00
	4.26
	5.27

	
	13
	2825
	4.23
	0.03
	1.47
	0.74
	1.60
	3.45
	4.91
	5.21
	5.48
	6.35

	
	14
	5621
	2.84
	0.02
	1.36
	0.24
	1.03
	1.48
	3.04
	3.91
	4.53
	5.56

	
	15
	6342
	1.64
	0.01
	0.78
	0.18
	0.61
	0.84
	1.78
	2.21
	2.58
	3.47

	
	16
	6342
	1.54
	0.01
	0.69
	0.20
	0.63
	0.77
	1.69
	2.04
	2.23
	3.06

	
	17
	6342
	1.75
	0.01
	0.78
	0.23
	0.71
	0.91
	2.00
	2.29
	2.62
	3.45

	
	18
	6038
	2.24
	0.01
	0.97
	0.26
	0.88
	1.29
	2.46
	3.00
	3.44
	3.94

	
	19
	5985
	3.47
	0.02
	1.26
	0.38
	1.37
	2.54
	3.77
	4.45
	4.94
	5.68

	
	20
	5624
	4.80
	0.02
	1.16
	0.57
	3.14
	4.52
	5.24
	5.45
	5.78
	6.31

	
	21
	4282
	2.98
	0.02
	1.47
	0.22
	0.92
	1.76
	3.27
	4.12
	4.75
	5.84

	
	22
	5294
	1.98
	0.01
	1.07
	0.22
	0.60
	1.12
	1.86
	2.98
	3.51
	3.81

	
	23
	5444
	2.20
	0.01
	1.01
	0.34
	0.78
	1.19
	2.27
	2.97
	3.57
	4.49

	
	24
	5757
	3.10
	0.02
	1.34
	1.00
	1.45
	1.84
	2.93
	4.16
	4.85
	7.00

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 









