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Figure S1. Schematic detailed overview of the Rozema PS. 
Table S1 Placement information of the 10 acoustic receivers 
	Receiver 
	Location name
	Lat 
	Long 
	Date placement   
	Date recovery

	R1
	Canal 1 
	53.28213
	7.004499
	24-8-2021
	19-1-2022 

	R2
	Side canal towards Delfzijl
	53.29359
	7.000795
	24-8-2021 
	19-1-2022 

	R3
	Canal 2
	53.29602
	7.024892
	24-8-2021 
	19-1-2022 

	R4
	Old sluice 
	53.30114
	7.033437
	18-8-2021 
	19-1-2022 

	R5
	Canal 3
	53.30049
	7.035373
	24-8-2021 
	19-1-2022 

	R6
	Shipping sluice
	53.30148
	7.036786
	18-8-2021 
	19-1-2022 

	R7
	Entrance fish passage 
	53.30223
	7.037271
	18-8-2021 
	2-2-2022 

	R8
	Saltwater side  
	53.30332
	7.037069
	18-8-2021 
	2-2-2022 

	R9
	Before pumping station Rozema
	53.30307
	7.038893
	24-8-2021 
	16-2-2022 

	R10
	After pumping station Rozema
	53.30307
	7.038893
	18-8-2021 
	2-2-2022 



Table S2. Number of eels detected on receivers in this and other projects. European Tracking Network – data management platform. Flanders Marine Institute, 2024, http://www.lifewatch.be/etn/, accessed 10-05-2024. 
	Project area and ETN acronym
	Project citation 
	Latitude 
	Longitude 
	Number of eels detected 

	Termunterzijl- current project RBVV2: Clear way for fish 2
	Huisman, J.; van Eerbeek J.; van der Knaap, I.; Van Hall Larenstein: Ruim baan voor vis 2; 2021. https://marineinfo.org/doc/dataset/7822
	53.343294
	6.967318

	40 

	Ems-Dollard 
RBVV2: Clear way for fish 2
	Huisman, J.; van Eerbeek J.; van der Knaap, I.; Van Hall Larenstein: Ruim baan voor vis 2; 2021. https://marineinfo.org/doc/dataset/7822
	53.343294
	6.967318

	32

	Wadden Sea Swimways_2021 
	Edwards, J.; 2021; Wadden Tools – Swimway Wadden Sea. 
https://marineinfo.org/doc/dataset/8030
	53.1666050000
	53.1666050000
	1

	North Sea ORSTEDCOD
	Winter, Erwin. (2021). ORSTED COD project. 
https://marineinfo.org/doc/dataset/6716
	51.6070000000
	3.0300000000

	2

	North Sea 
BPNS
	Reubens, J.; Hernandez, F; Deneudt, K.; (2017): LifeWatch observatory - Permanent acoustic receiver network in the Belgian Part of the North Sea. 
https://marineinfo.org/doc/dataset/5843
	51.4632100000

	2.7213200000

	1
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Figure S3. Image of one of the screw pumps at PS Rozema. 
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