Supplementary Method
Next-generation sequencing
· The detailed table for RNA quality control was provided, indicating that the RIN value from samples with grades A and B was RIN value ≥ 6.5，28S(25s)/18S ≥ 1.0.
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· The following are the details of the sequencing:
Sequencing machine: DNBSEQ-T7
Single-end or Paired-end: Paired-end
Read length: PE100
Read depth: Sequencing data volume > 100 million, Mapped rate > 90%
Was it mRNA poly-A enriched: yes.

· The quality control we conducted on the sequencing data：
The high-throughput sequencer generates raw image data files, which are then transformed into raw sequencing sequences through base calling and analysis. These raw sequences are referred to as raw data. To ensure the quality of information analysis, the software fastp is used to remove adapter sequences, filter out low-quality bases, and N bases (representing undetermined bases), resulting in high-quality clean data. The clean data is then subjected to statistical analysis, including the number of bases and sequences. The specific filtering criteria are as follows:
1) Removal of reads with a length less than 35bp after trimming adapter sequences and low-quality bases at both ends.
2) Removal of reads with an N (N represents undetermined base information) proportion greater than 10% of the total number of bases.
3) Removal of reads with a proportion of low-quality bases (quality value Q ≤ 5) accounting for more than 40% of the entire read length in single-end reads.
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Sequencing type Quantity concentration purity integrity determination result sample grade
Meeting concentration and
=400ng =5ng/ul electrophoresis quality control, and it is A
RIN=6.5 sufficient for 2 library preparations.
285(25s)/18521.0 Meeting concentration and
>200ng =5ng/ul No DNA, protein, or saltion electrophoresis quality control, and itis B
Eukaryotic contamination.The sample sufficient for 1 library preparations.
transcriptome 1S colocrjless, fransparent, The sample quality partially meets the
and non-viscous; ; ; ;
library - mRNA : 6 <RIN<6.5, requirements for library preparation and
100 < RNA <200ng 22ng/ul 0D260/28021.8 285(25s)/[185=21.0 sequencing, and library construction C
0D260/23022.0 can be attempted.
The sample quality does not meet the
RIN <6 requirements for library preparation and D

<100ng

sequencing at all, and itis not
recommended to use this sample.











