Supplementary
A 	Completion of the geothermal wells at Schäftlarnstraße that were used for the FO-monitoring system.
	Well 1 (Producer)
	Depth [m MD]
	Depth [m TVD]
	Completion
	KOP [m MD]
	Inclination

	
	870
	870
	20 inch
	250
	4°

	 
	2010
	1812
	13 3/8 inch
	880
	44°

	 
	2819
	2408
	[bookmark: _GoBack]9 5/8 inch
	2220
	42°

	 
	3741
	2947
	7 inch
	2850
	58°

	Well 2 (Injector)
	Depth [m MD]
	Depth [m TVD]
	Completion
	KOP [m MD]
	Inclination

	
	880
	880
	20 inch
	250
	4°

	 
	2311
	1980
	13 3/8 inch
	880
	44°

	 
	3345
	2610
	9 5/8 inch
	2220
	42°

	 
	4443
	2723
	Open Hole
	2850
	58°





