Structural control of the graben fault on hydrothermal alteration in the Cerro Pabellón geothermal system (Andean Cordillera, Northern Chile)
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Table S1 Structural formula of saponite at 470 and 700m in CP5A well and at 1400m depth in CP2A well. n.a.: number of analyses; an. ave.: analytical average; s.d.: standard deviation. OCT: octahedral occupancy; INTCH: interlayer charge;. The formulas are normalized to 11 O atoms and total Fe is considered as Fe2+.
	depth
	CP5A 470
	CP5A 700
	CP2A 1400

	mineral
	sap
	sap
	sap

	n.a
	7
	3
	6

	
	an. ave.
	s.d.
	an. ave.
	s.d.
	an. ave.
	s.d.

	Si
	3,09
	0,04
	3,39
	0,01
	3,30
	0,12

	Al
	1,19
	0,02
	0,73
	0,02
	0,81
	0,09

	Fe2+
	0,35
	0,03
	1,00
	0,05
	0,62
	0,12

	Mg
	2,27
	0,09
	1,83
	0,05
	2,31
	0,14

	Ti
	0,01
	0,02
	0,00
	0,00
	0,00
	0,00

	Mn
	0,04
	0,00
	0,02
	0,00
	0,02
	0,00

	OCT
	2,95
	0,08
	2,96
	0,02
	3,06
	0,11

	Na
	0,06
	0,01
	0,04
	0,01
	0,11
	0,08

	Ca
	0,30
	0,05
	0,25
	0,02
	0,17
	0,06

	K
	0,05
	0,01
	0,03
	0,01
	0,02
	0,00

	INTCH
	0,71
	0,11
	0,57
	0,04
	0,80
	0,02

	Fe/(Fe+Mg)
	0,13
	0,01
	0,35
	0,02
	0,21
	0,04

	Si/(Si+Al)
	0,72
	0,03
	0,82
	0,03
	0,80
	0,02



Table S2 Structural formula of corrensite and C-Crr mixed layers at 470 and 700m depth in CP5A well and C-Crr mixed layers at 1400m depth in CP2A. n.a.: number of analyses; an. ave.: analytical average; s.d.: standard deviation. OCT: octahedral occupancy; INTCH: interlayer charge;. The formulas are normalized to 25 O atoms and total Fe is considered as Fe2+.
	depth
	CP5A 470
	CP5A 470
	CP5A 700
	CP2A 1400

	mineral
	crr
	c-crr
	c-crr
	c-crr

	n.a
	23
	5
	17
	17

	
	an. ave.
	s.d.
	an. ave.
	s.d..
	an. ave.
	s.d.
	an. ave.
	s.d.

	Si
	6,40
	0,32
	6,20
	0,17
	5,78
	0,05
	6,54
	0,01

	Al
	3,03
	0,30
	3,15
	0,30
	4,53
	0,16
	2,57
	0,02

	Fe2+
	1,28
	0,73
	2,34
	0,08
	2,23
	0,18
	1,51
	0,33

	Mg
	5,99
	0,49
	5,26
	0,23
	4,24
	0,15
	6,29
	0,34

	Ti
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00

	Mn
	0,10
	0,03
	0,07
	0,01
	0,05
	0,01
	0,05
	0,00

	OCT
	9,05
	0,37
	9,88
	0,06
	9,69
	0,12
	9,82
	0,01

	Na
	0,08
	0,03
	0,05
	0,01
	0,02
	0,01
	0,10
	0,06

	Ca
	0,22
	0,07
	0,15
	0,02
	0,08
	0,01
	0,15
	0,00

	K
	0,05
	0,02
	0,06
	0,04
	0,04
	0,01
	0,02
	0,00

	INTCH
	0,57
	0,13
	0,40
	0,04
	0,23
	0,01
	0,41
	0,06

	Fe/(Fe+Mg)
	0,17
	0,09
	0,55
	0,03
	0,34
	0,01
	0,35
	0,08

	Si/(Si+Al)
	0,68
	0,03
	3,63
	0,41
	0,56
	0,01
	1,28
	0,00


Table S3 Structural formula of chlorite at 445 and 700 m depth in CP5A well and 1400, 1530 and 1540m depth in CP2A well. n.a.: number of analyses; an. ave.: analytical average; s.d.: standard deviation. OCT: octahedral occupancy; INTCH: interlayer charge;. The formulas are normalized to 14 O atoms and total Fe is considered as Fe2+. 
	depth
	CP5A 445
	CP5A 700
	CP2A 1400
	CP2A 1530
	CP2A 1540

	mineral
	chl
	chl
	chl
	chl
	chl

	n.a
	26
	23
	6
	4
	4

	
	an. ave.
	s.d.
	an. ave.
	an. ave.
	an. ave.
	an. ave.
	an. ave.
	an. ave.
	an. ave.
	an. ave.

	Si
	3,14
	0,12
	3,15
	0,09
	3,39
	0,17
	3,06
	0,10
	3,23
	0,04

	Al
	2,23
	0,06
	2,10
	0,19
	1,81
	0,24
	2,17
	0,15
	2,32
	0,06

	Fe2+
	1,62
	0,18
	1,60
	0,14
	1,07
	0,28
	1,78
	0,25
	1,38
	0,07

	Mg
	2,56
	0,19
	2,84
	0,12
	3,33
	0,28
	2,73
	0,29
	2,56
	0,11

	Ti
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00
	0,01
	0,00
	0,00
	0,00

	Mn
	0,13
	0,07
	0,06
	0,01
	0,02
	0,01
	0,04
	0,02
	0,03
	0,00

	OCT
	5,68
	0,15
	5,75
	0,04
	5,63
	0,11
	5,79
	0,06
	5,52
	0,08

	Na
	0,03
	0,04
	0,01
	0,01
	0,04
	0,03
	0,04
	0,06
	0,03
	0,01

	Ca
	0,02
	0,01
	0,04
	0,01
	0,05
	0,02
	0,03
	0,02
	0,05
	0,01

	K
	0,05
	0,02
	0,01
	0,01
	0,02
	0,01
	0,01
	0,01
	0,06
	0,03

	INTCH
	0,12
	0,06
	0,10
	0,02
	0,15
	0,08
	0,11
	0,09
	0,18
	0,03

	Fe/(Fe+Mg)
	0,39
	0,03
	0,36
	0,03
	0,24
	0,06
	0,40
	0,06
	0,35
	0,01

	Si/(Si+Al)
	0,59
	0,01
	1,52
	0,19
	0,65
	0,04
	0,58
	0,03
	0,58
	0,00



Table S4 Structural formula of illitic minerals at 445m, 470m, 550m and 700m depth in CP5A well and 1530 and 1540m depth in CP2A well. n.a.: number of analyses; an. ave.: analytical average; s.d.: standard deviation. OCT: octahedral occupancy; INTCH: interlayer charge;. The formulas are normalized to 11 O atoms and total Fe is considered as Fe3+.
	depth
	CP5A 445
	CP5A 470
	CP5A 550
	CP5A 700

	mineral
	illitic minerals
	illitic minerals
	illitic minerals
	illitic minerals

	n.a
	9
	9
	14
	11

	
	an. ave.
	s.d.
	an. ave.
	s.d.
	an. ave.
	s.d.
	an. ave.
	s.d.

	Si
	3,36
	0,08
	3,40
	0,07
	3,46
	0,03
	3,39
	0,01

	Al IV
	0,64
	0,08
	0,60
	0,07
	0,54
	0,03
	0,61
	0,01

	Al VI
	1,75
	0,04
	1,60
	0,07
	1,55
	0,10
	1,79
	0,02

	Fe3+
	0,10
	0,02
	0,14
	0,03
	0,19
	0,07
	0,08
	0,01

	Mg
	0,12
	0,04
	0,23
	0,05
	0,22
	0,04
	0,11
	0,01

	Ti
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00

	Mn
	0,00
	0,01
	0,00
	0,00
	0,00
	0,00
	0,00
	0,00

	OCT
	1,97
	0,01
	1,97
	0,02
	1,97
	0,01
	1,99
	0,01

	Na
	0,03
	0,01
	0,04
	0,02
	0,02
	0,01
	0,03
	0,01

	Ca
	0,01
	0,01
	0,01
	0,01
	0,02
	0,01
	0,01
	0,01

	K
	0,79
	0,08
	0,86
	0,07
	0,79
	0,02
	0,70
	0,03

	INTCH
	0,84
	0,07
	0,92
	0,06
	0,85
	0,02
	0,76
	0,03





	depth
	CP2A 1530
	CP2A 1540

	mineral
	illitic minerals
	illitic minerals

	n.a
	6
	7

	
	an. ave.
	s.d.
	an. ave.
	s.d.

	Si
	3,36
	0,02
	3,44
	0,07

	Al IV
	0,64
	0,02
	0,56
	0,07

	Al VI
	1,81
	0,01
	1,65
	0,09

	Fe3+
	0,11
	0,01
	0,18
	0,06

	Mg
	0,11
	0,01
	0,23
	0,04

	Ti
	0,00
	0,00
	0,00
	0,00

	Mn
	0,00
	0,00
	0,00
	0,00

	OCT
	2,03
	0,02
	2,06
	0,02

	Na
	0,04
	0,01
	0,04
	0,01

	Ca
	0,01
	0,02
	0,03
	0,01

	K
	0,70
	0,01
	0,68
	0,02

	INTCH
	0,76
	0,05
	0,78
	0,02



