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Additional File 2
a) Hourly means of measured CO2 concentration (ppm; Log10 scale) at 2 m from the ground (red solid line) vs hourly simulation output (blue solid line) obtained with Kzmin=0, considering the mean gas flux (sim2, Φd mean, Table 3) for a) station V11, b) station V202, and c) station V08. Red vertical bars represent the standard deviation associated to the means of observed data.  
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