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Figure S1 Discrepancy between estimated and true prism heights obtained by varying the initial model. Upper figures represent the true models, and the lower ones show the relationships between the mean height difference and the initial depths of the boundaries. a The thickness of the shallower low-density layer is thinner than that in the model in the main body. The depth difference between the deep and shallow boundaries, i.e., the middle layer thickness, is up to approximately 1200 m. b The thickness of the shallower low-density layer is greater than that in the model in the main body. The depth difference between the deep and shallow boundaries, i.e., the middle layer thickness, is up to approximately 300 m.
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