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Figure S1 Rheological properties of pure alginate gel pastes: a) results of the flow tests and b) results of the three-step flow recovery tests.
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