Table S1 Instrument operation program of UPLC-MS/MS analysis 

	Team
	Parameter
	Item
	Parameter

	Column temperature
	30 ℃
	Mass range
	80 m/z to 1200 m/z

	Autosampler temperature
	4 ℃
	Sheath gas flow rate
	30 psi

	Sample injection volume
	2 µl
	Auxiliary gas flow rate
	10 psi

	Mobile phase A
	Water plus 0.1% formic acid
	Transmission Capillary temperature
	320 ℃

	Mobile phase B
	Methanol
	Primary scan resolutions
	70 000

	Spray voltage
	3.0 kV
	Secondary scan resolutions
	17500


