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1. [bookmark: _Toc159313016]Figure S1: 68Ga-labeling of [68Ga]Ga-FR and [68Ga]Ga-FRH
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Popis byl vytvořen automaticky]
Figure S1A: Example of radiochromatogram of [68Ga]Ga-FR.
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Figure S1B: Example of radiochromatogram of [68Ga]Ga-FRH.
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Popis byl vytvořen automaticky]Figure S2: Quality control of [68Ga]Ga-FR and [68Ga]Ga-FRH on radio-iTLC-SG 
  68GaCl3 generator eluate      [68Ga]Ga-FR
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Popis byl vytvořen automaticky]Figure S2A: Radiochromatograms of 68GaCl3 generator eluate and [68Ga]Ga-FR in ammonium acetate (1M)  and methanol (1:1). 
68GaCl3 generator eluate                 [68Ga]Ga-FRH



[bookmark: _GoBack]Figure S2B: Radiochromatograms of 68GaCl3 generator eluate and [68Ga]Ga-FR in ammonium acetate (1M)  and methanol (1:1).
[bookmark: _Toc159313018]3. Figure S3: In vivo stability tests
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Popis byl vytvořen automaticky]
Figure S3A: Radiochromatogram of [68Ga]Ga-FR stability in blood, 5 min after injection.
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Popis byl vytvořen automaticky]
Figure S3B: Radiochromatogram of [68Ga]Ga-FRH stability in blood, 5 min after injection.
[image: Obsah obrázku řada/pruh, snímek obrazovky, diagram, text

Popis byl vytvořen automaticky]
Figure S3C: Radiochromatogram of [68Ga]Ga-FR stability in urine, 30 min after injection.
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Figure S3D: Radiochromatogram of [68Ga]Ga-FR stability in urine, 90 min after injection.
[image: ]
Figure S3E: Radiochromatogram of [68Ga]Ga-FRH stability in urine, 30 min after injection.
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Figure S3F: Radiochromatogram of [68Ga]Ga-FRH stability in urine, 90 min after injection.
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