Video.1：Surgical video through AR vision using HMD.
1. Before setting up the surgical field, the hologram was overlaid on the patient’s radius through the HMD in advance.
2, After the surgical field was deployed, the position of the hologram was adjusted against the radius.
3, Two 1.2 mm Kirshner wires were inserted into the radius in alignment with the osteotomy plane of the superimposed AR guide.
4, Use the Hologram was used and Kirschner wires were inserted as guides to perform osteotomy with a bone saw. 
5．The iliac bone was harvested and shaped according to the hologram of the bone-graft model.



2

