Supplementary materials
The improvement of dispersity, thermal stability and mechanical properties of collagen fibers by silane modification: An exploration for developing new leather making technology
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Figure S1 CF, TMS12-CF, TMS16-CF and TMS18-CF were immersed in water
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Figure S2 TMS16-CF (a) and TMS18-CF (b) were immersed in solution with different pH.
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Figure S3 DSC curve of CF.
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