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Calibration curve to express the measurements in Field capacity.
The values recorded were used to calculate FC % as follows:  
FC= [(Ww-Wdry) * 100%] / ( X * Fcorr)
where Ww is the current wet weight; Wdry is the dry weight of the soil mixture before being saturated; X is the g of water uptaken per 100 g of mixture; Fcorr is a correction factor expressed in g-1 to normalize all pots. 

