Table S2. Properties of samplers.
	Sampler (material)
	Manufacturer
	Dimensions
	Sample area
	MPmin
	MPmax

	
	
	Height
	Width
	Length
	
	
	

	Van Veen grab sampler (stainless steel)
	Hydro-Bios, Altenholz, Germany
	60 cm
	25 cm
	20 cm
	250 cm2
	121
	100

	Sediment corer (stainless steel)
	Hydro-Bios, Altenholz, Germany
	Outer diameter: 10 cm
Inner diameter: 7.2 cm 
	100 cm
	41 cm2
	12
	32

	Stainless steel shovel
	Denios AG, Bad Oeynhausen, Germany
	11.5 cm
	10 cm
	19.5 cm
	195 cm2
	91
	112

	Percussion corer (steel, PVC)
	Eijkelkamp, Giesbeek, The Netherlands
	Liner: 5 cm outside and 4.6 cm inside
Probe pole: 
6.2 cm outside and 
5.8 cm inside
Core catcher (stainless steel): 4.6 cm
	133 cm
	16.62 cm2
	7
	12

	Freeze corer (steel, copper)
	-
	Outer diameter: 2 cm
Inner diameter: 1 cm
	104 cm
	-
	Depends on diameter of freeze core obtained



