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Table S1 Research vessels used for microplastic particles sampling in Tokyo Bay during October–November 2023.
	Sampling date
(YYYYMMDD)
	Stations
	Vessel name
	Gross tonnage
(t)
	Length
(m)

	20231027
	St. 1, 2, 4
	Target
	<5
	6.14

	20231108
	St. 3, 5, 6
	MAKOTOMARU
	2.0
	8.5

	20231129
	St. 7, 8
	Tokyo Bay · hⅡ
	1.5
	6.77





Table S2 Polymer types identified in this study and their density ranges.
	Polymer name
	Abbreviation
	 Density (g/cm3)*

	acrylonitrile-butadiene-styrene
	ABS
	0.99-1.15 [1]

	alkyd resin
	alkyd
	1.10-1.46 [2]

	polyacrylate styrene
	AS
	1.08-1.1 [1]

	epoxy resin
	epoxy
	1.11-1.40 [2]

	polyamide
	PA
	1.12-1.14 [1]

	polyethylene
	PE
	0.91-0.97 [1]

	polyethylene terephthalate
	PET
	1.38-1.39 [1]

	polymethyl methacrylate & polymethyl acrylate
	PMMA
	1.17-1.20 [1]

	polypropylene
	PP
	0.90-0.91 [1]

	polystyrene
	PS
	1.04-1.07 [1]

	polyurethane
	PU
	1.20 [1]

	polyvinyl acetate
	PVAc
	1.19 [3]

	polyvinyl chloride
	PVC
	1.16-1.35 [1]

	styrene-butadiene rubber
	SBR
	0.93-0.94 [4]


Note: The average of the minimum and maximum reported density values was used for each polymer type in this study.

1. https://kayo-corp.co.jp/common/pdf/pla_propertylist01.pdf 
2. https://kayo-corp.co.jp/common/pdf/pla_propertylist02.pdf 
3. https://pubchem.ncbi.nlm.nih.gov/#query=Polyvinyl-acetate 
4. https://kayo-corp.co.jp/common/pdf/rub_propertylist.pdf
Table S3 Summary of previous studies on microplastic particles collected from the surface water of Tokyo Bay.
	Reference
	Sampling date
	Sampling method
	Digestion
	Density separation (g/cm3)
	Size range (μm)
	Concentration
(particles/L)
	Identification
	Main type
	Main shape

	Nakano et al. (2021)
	May 2019,
Jan 2020
	5 sites, Neuston net (350 µm mesh),
Depth of 0–75 cm
	H2O2+
Fenton reaction
	1.5 (NaI)
	≥ 100
	0.00004–0.0178
	ATR-FTIR
	PE, PP
	Fragment

	Xu et al. (2022)
	Dec 2020
	2 sites, Double neuston net (inner net: 350 µm, outer net: 50 µm),
Depth of 0–75 cm
	H2O2+
Fenton reaction
	1.6 (NaI)
	50–350
≥ 350
	3.06–3.22
0.00247–0.0205
	μ-FTIR
ATR-FTIR
	Co-polymer, PE, PP 
Co-polymer, PE, PP
	Fragment
Fragment

	Sato et al. (2024)
	July 2021
	2–6 sites, Double neuston net (inner net: 350 µm, outer net: 50 µm),
Depth of 0–75 cm
	H2O2+ Fenton reaction
	1.6 (NaI)
	60–350
≥ 350
	0.80–11.5
0.00021–0.00334
	μ-FTIR
ATR-FTIR
	Co-polymer, PE 
Co-polymer, PE, PP
	Fragment
Fragment

	Sato et al. (2024)
	July 2021
	6 sites, Plankton pump with 60 µm mesh,
Depth of 200 cm
	H2O2+ Fenton reaction
	1.6 (NaI)
	60–350
	0.36–5.79
	μ-FTIR
	Co-polymer, PE 
	Fragment

	Ueda et al.
(2025)
	Dec 2022
	4 sites, Hand pump and filtered with 10µm mesh plankton net,
Depth of 30–50 cm
	H2O2
	1.7 (NaI)
	≥ 20
20–100
100–350
≥ 350
	0.698–27.3
0.545–23.7
0.116–3.31
0.0372–0.171
	μ-FTIR
μ-FTIR
μ-FTIR
μ-FTIR
	PE, PET, PMMA, PP
PE, PET, PMMA, PP
PE, PET, PMMA, PP
PET
	Fragment
Fragment
Fragment
Fiber

	This study
	Oct–Nov 2023
	8 sites, Submersible pump and filtered with 10µm mesh plankton net,
Depth of 50 cm
	H2O2
	1.7 (NaI)
	≥ 20
20–100
100–350
≥ 350
	0.835–11.3
0.564–8.10
0.235–2.86
0.0325–0.349
	μ-FTIR
μ-FTIR
μ-FTIR
μ-FTIR
	PE, PET, PMMA, PP
PE, PET, PMMA, PP
PE, PET, PMMA, PP
PET
	Fragment
Fragment
Fragment
Fiber



Table S4 Size-fractionated concentrations and composition of microplastic particles in surface water samples collected from eight stations in Tokyo Bay in 2023, based on measured particle counts and estimated particle mass.
	Station
	Number-based concentrations (particles/L)
	
	Estimated mass-based concentrations (µg/L)

	
	20–100 µm
	100–350 µm
	≥ 350 µm
	Total
	
	20–100 µm
	100–350 µm
	≥ 350 µm
	Total

	St. 1
	8.10
(71.6%)
	2.86
(25.3%)
	0.35
(3.1%)
	11.31
	
	0.30
(14.9%)
	1.55
(76.4%)
	0.18
(8.7%)
	2.03

	St. 2
	0.87
(65.2%)
	0.40
(29.9%)
	0.08
(4.9%)
	1.35
	
	0.04
(0.5%)
	0.24
(2.9%)
	7.96
(96.6%)
	8.24

	St. 3
	1.66
(64.4%)
	0.71
(27.6%)
	0.21
(8.0%)
	2.58
	
	0.09
(14.6%)
	0.50
(77.5%)
	0.05
(7.9%)
	0.64

	St. 4
	0.56
(67.5%)
	0.24
(28.6%)
	0.03
(3.9%)
	0.84
	
	0.04
(15.8%)
	0.09
(41.3%)
	0.10
(42.9%)
	0.23

	St. 5
	0.97
(77.9%)
	0.24
(18.8%)
	0.04
(3.4%)
	1.25
	
	0.05
(4.5%)
	0.15
(12.9%)
	0.98
(82.6%)
	1.19

	St. 6
	4.88
(83.8%)
	0.88
(15.1%)
	0.07
(1.1%)
	5.82
	
	0.16
(30.7%)
	0.35
(66.9%)
	0.01
(2.3%)
	0.52

	St. 7
	2.74
(69.3%)
	1.11
(28.0%)
	0.11
(2.7%)
	3.95
	
	0.17
(21.1%)
	0.50
(61.1%)
	0.15
(17.8%)
	0.82

	St. 8
	1.43
(74.8%)
	0.38
(19.8%)
	0.10
(5.4%)
	1.91
	
	0.10
(14.2%)
	0.23
(33.6%)
	0.36
(52.2%)
	0.69

	Mean ± SD
	2.36 ± 2.59
(71.8 ± 6.7%)
	0.85 ± 0.87
(24.1 ± 5.5%)
	0.12 ± 0.11
(4.1 ± 2.1%)
	3.63 ± 3.52
	
	0.12 ± 0.09
(17.6 ± 11.1%)
	0.45 ± 0.47
(43.6 ± 25.1%)
	1.22 ± 2.74
(38.7 ± 35.9%)
	1.79 ± 2.66


Note: Percentages in parentheses indicate the proportion of microplastic particles in each category of each size relative to the total concentration.

Table S5 Size-specific morphological composition of microplastic particles in surface water samples collected from eight stations in Tokyo Bay in 2023.
	Station
	Number-based (%)
	
	Estimated mass-based (%)

	
	20–100 µm
	100–350 µm
	≥ 350 µm
	Total
	
	20–100 µm
	100–350 µm
	≥ 350 µm
	Total

	
	Frag.
	Fib.
	Frag.
	Fib.
	Frag.
	Fib.
	Frag.
	Fib.
	
	Frag.
	Fib.
	Frag.
	Fib.
	Frag.
	Fib.
	Frag.
	Fib.

	St. 1
	98.3%
	1.7%
	82.9%
	17.1%
	ND
	100%
	98.3%
	1.7%
	
	99.4%
	0.6%
	97.6%
	2.4%
	ND
	100%
	89.4%
	10.6%

	St. 2
	99.1%
	0.9%
	85.7%
	14.3%
	35.0%
	65.0%
	91.5%
	8.5%
	
	99.98%
	0.02%
	90.2%
	9.8%
	99.7%
	0.3%
	99.6%
	0.4%

	St. 3
	100%
	ND
	95.8%
	4.2%
	ND
	100%
	90.8%
	9.2%
	
	100%
	ND
	99.2%
	0.8%
	ND
	100%
	91.4%
	8.6%

	St. 4
	100%
	ND
	81.8%
	18.2%
	33.3%
	66.7%
	92.2%
	7.8%
	
	100%
	ND
	95.1%
	4.9%
	90.7%
	9.3%
	94.0%
	6.0%

	St. 5
	99.1%
	0.9%
	85.7%
	14.3%
	23.6%
	76.4%
	94.0%
	6.0%
	
	99.8%
	0.2%
	98.6%
	1.4%
	99.2%
	0.8%
	99.2%
	0.8%

	St. 6
	98.2%
	1.8%
	74.1%
	25.9%
	ND
	100%
	93.5%
	6.5%
	
	99.4%
	0.6%
	95.8%
	4.2%
	ND
	100%
	94.7%
	5.3%

	St. 7
	100%
	ND
	81.0%
	19.0%
	ND
	100%
	97.1%
	8.0%
	
	100%
	ND
	97.9%
	2.1%
	ND
	100%
	80.9%
	19.1%

	St. 8
	100%
	ND
	77.3%
	22.7%
	50.0%
	50.0%
	92.8%
	7.2%
	
	100%
	ND
	97.7%
	2.3%
	96.0%
	4.0%
	97.2%
	2.8%

	Mean ± SD
	99.3 ± 0.8%
	0.7 ± 0.8%
	83.0 ± 6.5%
	17.0 ± 6.5%
	17.7 ± 20.3%
	82.3 ± 20.3%
	92.9 ± 2.0%
	7.7 ± 1.1%
	
	99.8 ± 0.3%
	0.2 ± 0.3%
	96.5 ± 2.9%
	3.5 ± 2.9%
	48.2 ± 51.6%
	51.8 ± 51.6%
	93.3 ± 6.2%
	6.7 ± 6.2%


Note: Percentages in parentheses indicate the proportion of microplastic particles in each size category relative to the total concentration.
ND = Not detected.

Table S6 Relative composition of microplastic polymer types by particle count in surface water samples collected from eight stations in Tokyo Bay during October–November 2023.
	Polymer type
	St. 1
	St. 2
	St. 3
	St. 4
	St. 5
	St. 6
	St. 7
	St. 8
	Mean ± SD
	Num. of
detected
stations

	alkyd
	ND
	1.8%
	8.0%
	10.4%
	1.3%
	0.2%
	ND
	ND
	2.7 ± 4.1%
	5

	AS
	ND
	0.2%
	ND
	ND
	ND
	0.6%
	ND
	ND
	0.1 ± 0.2%
	2

	epoxy
	ND
	1.2%
	1.1%
	ND
	ND
	0.2%
	ND
	ND
	0.3 ± 0.5%
	3

	PA
	1.9%
	ND
	ND
	ND
	0.7%
	0.2%
	ND
	1.8%
	0.6 ± 0.8%
	4

	PE
	29.0%
	26.6%
	26.4%
	41.6%
	24.8%
	2.6%
	10.7%
	26.1%
	23.6 ± 11.9%
	8

	PET
	11.7%
	10.8%
	20.7%
	19.5%
	16.1%
	4.1%
	16.0%
	7.2%
	13.3 ± 5.8%
	8

	PMMA
	7.4%
	36.9%
	18.4%
	10.4%
	28.1%
	70.0%
	50.6%
	45.0%
	33.4 ± 21.5%
	8

	PP
	49.4%
	18.8%
	20.7%
	11.7%
	27.6%
	21.8%
	22.7%
	16.2%
	23.6 ± 11.4%
	8

	PS
	ND
	0.6%
	ND
	ND
	0.7%
	ND
	ND
	ND
	0.2 ± 0.3%
	2

	PU
	ND
	ND
	1.1%
	1.3%
	ND
	ND
	ND
	ND
	0.3 ± 0.6%
	2

	PVAc
	ND
	ND
	2.3%
	1.3%
	ND
	ND
	ND
	ND
	0.4 ± 0.9%
	2

	PVC
	0.6%
	3.0%
	1.1%
	3.9%
	0.7%
	0.4%
	ND
	3.6%
	1.7 ± 1.6%
	7


Note: ND = Not detected.

Table S7 Relative composition of microplastic polymer types by estimated mass in surface water samples collected from eight stations in Tokyo Bay during October–November 2023.
	Polymer type
	St. 1
	St. 2
	St. 3
	St. 4
	St. 5
	St. 6
	St. 7
	St. 8
	Mean ± SD
	Num. of
detected
stations

	alkyd
	ND
	3.4%
	11.6%
	15.2%
	0.2%
	2.2%
	ND
	ND
	4.1 ± 6.0%
	5

	AS
	ND
	1.1%
	ND
	ND
	ND
	1.2%
	ND
	ND
	0.3 ± 0.5%
	2

	epoxy
	ND
	0.1%
	24.3%
	ND
	ND
	0.05%
	ND
	ND
	3.1 ± 8.6%
	3

	PA
	0.1%
	ND
	ND
	ND
	2.5%
	0.2%
	ND
	0.3%
	0.4 ± 0.9%
	4

	PE
	24.9%
	0.9%
	18.6%
	20.2%
	1.9%
	0.9%
	9.3%
	7.0%
	10.5 ± 9.6%
	8

	PET
	13.8%
	89.3%
	21.6%
	12.9%
	9.1%
	2.8%
	50.0%
	22.4%
	27.7 ± 28.6%
	8

	PMMA
	7.9%
	1.9%
	6.8%
	6.9%
	3.3%
	80.3%
	30.3%
	65.9%
	25.4 ± 31.0%
	8

	PP
	42.3%
	0.2%
	6.8%
	2.9%
	83.0%
	11.7%
	10.4%
	2.8%
	20.0 ± 28.7%
	8

	PS
	ND
	0.002%
	ND
	ND
	0.04%
	ND
	ND
	ND
	0.01 ± 0.01%
	2

	PU
	ND
	ND
	0.4%
	0.5%
	ND
	ND
	ND
	ND
	0.1 ± 0.2%
	2

	PVAc
	ND
	ND
	0.1%
	0.8%
	ND
	ND
	ND
	ND
	0.1 ± 0.3%
	2

	PVC
	11.0%
	3.1%
	9.8%
	40.6%
	0.1%
	0.6%
	ND
	1.6%
	8.3 ± 13.7%
	7


[bookmark: _Hlk203398801]Note: ND = Not detected.

Table S8 Summary of previous studies on microplastic particles in sediment samples from Tokyo Bay.
	Reference
	Sampling date
	Sampling method
	Digestion
	Density separation (g/cm3)
	Size range (μm)
	Concentration
(particles/g D.W.)
	Identification
	Main type
	Major shape

	Matsuguma et al. (2017)
	Jul. 2012
	1 site, Gravity corer, 5 cm sliced intervals, sediment core 0–30 cm
	 H2O2
	1.6 NaI
	≥ 315
	1.845–5.385
	ATR-FTIR
	PAK, PCL, PE, PEP, PET, PS 
	Fragment

	Wang et al. (2021)
	May 2019, 
Jan 2020
	3 sites, Ekman–Birge sampler, upper 0–5 cm sediment
	H2O2
	1.6 NaI
	≥ 25
	53.3–148
	μ-FTIR
	Copolymer, PA, PE, PP 
	Fragment

	Hashim et al. (2024)
	Jul. 2021
	4 sites, Columnar mud collector, upper 0–5 cm sediment
	H2O2 + Fenton reaction
	1.6 NaI
	≥ 20
	11.5–21.1
	μ-FTIR
	Copolymer, PA, PE, PP 
	–

	This study
	Oct–Nov 2023
	8 sites, Ekman–Birge sampler, upper 0–10 cm sediment
	H2O2 + Fenton reaction
	1.7 NaI
	≥ 20
20–100
100–350
≥ 350
	37–268
31–253
2 –41
0–9
	μ-FTIR
μ-FTIR
μ-FTIR
μ-FTIR
	PE, PET, PMMA, PP
PE, PMMA, PP
PE, PP
PET
	Fragment
Fragment
Fragment
Fiber





Table S9 Size-fractionated concentrations and composition of microplastic particles in sediment samples collected from eight stations in Tokyo Bay in 2023, based on measured particle counts and estimated particle mass.
	Station
	Number-based concentrations (particles/g D.W.)
	
	Estimated mass-based concentrations (µg/g D.W.)

	
	20–100 µm
	100–350 µm
	≥ 350 µm
	Total
	
	20–100 µm
	100–350 µm
	≥ 350 µm
	Total

	St. 1
	31
(84.1%)
	3
(6.8%)
	3
(9.1%)
	37
	
	0.60
(19.0%)
	0.52
(16.6%)
	2.03
(64.4%)
	3.15

	St. 2
	118
(70.7%)
	41
(24.4%)
	8
(4.9%)
	167
	
	5.80
(18.7%)
	23.72
(76.6%)
	1.46
(4.7%)
	30.97

	St. 3
	107
(95.9%)
	2
(2.0%)
	2
(2.0%)
	112
	
	4.24
(86.4%)
	0.06
(1.2%)
	0.61
(12.4%)
	4.91

	St. 4
	133
(91.3%)
	11
(7.5%)
	2
(1.3%)
	145
	
	3.95
(14.6%)
	3.35
(12.4%)
	19.77
(73.0%)
	27.07

	St. 5
	253
(94.3%)
	15
(5.7%)
	0
(0.0%)
	268
	
	7.73
(27.1%)
	20.81
(72.9%)
	0
(0.0%)
	28.54

	St. 6
	75
(82.5%)
	7
(7.9%)
	9
(9.5%)
	91
	
	3.22
(40.2%)
	3.63
(45.3%)
	1.16
(14.5%)
	8.01

	St. 7
	63
(64.7%)
	31
(32.4%)
	3
(2.9%)
	97
	
	3.42
(19.4%)
	13.14
(74.7%)
	1.03
(5.8%)
	17.58

	St. 8
	43
(90.3%)
	5
(9.7%)
	0
(0.0%)
	48
	
	2.81
(58.1%)
	2.02
(41.9%)
	0
(0.0%)
	4.83

	Mean ± SD
	103 ± 71
(84.2 ± 11.5%)
	15 ± 15
(12.1 ± 10.8%)
	3 ± 3
(3.7 ± 3.3%)
	121 ± 74
	
	3.97 ± 2.11
(35.4 ± 25.2%)
	8.41 ± 9.50
(42.7 ± 30.3%)
	3.26 ± 6.71
(21.9 ± 29.5%)
	15.63 ± 11.84


Note: Percentages in parentheses indicate the proportion of microplastic particles in each category of each size relative to the total concentration.



Table S10 Size-specific morphological composition of microplastic particles in sediment samples collected from eight stations in Tokyo Bay in 2023.
	Station
	Number-based (%)
	
	Estimated mass-based (%)

	
	20–100 µm
	100–350µm
	≥ 350 µm
	
	20–100 µm
	100–350µm
	≥ 350 µm

	
	Fragment
	Fiber
	Fragment
	Fiber
	Fragment
	Fiber
	
	Fragment
	Fiber
	Fragment
	Fiber
	Fragment
	Fiber

	St. 1
	97.3%
	2.7%
	33.3%
	66.7%
	ND
	100%
	
	96.9%
	3.1%
	77.0%
	23.0%
	ND
	100%

	St. 2
	100%
	ND
	90.0%
	10.0%
	ND
	100%
	
	100%
	ND
	99.3%
	0.7%
	ND
	100%

	St. 3
	97.9%
	2.1%
	ND
	100%
	ND
	100%
	
	99.2%
	0.8%
	ND
	100%
	ND
	100%

	St. 4
	98.6%
	1.4%
	66.7%
	33.3%
	100
	ND
	
	99.2%
	0.8%
	97.9%
	2.1%
	100%
	ND

	St. 5
	97.6%
	2.4%
	60.0%
	40.0%
	ND
	ND
	
	99.1%
	0.9%
	99.3%
	0.7%
	ND
	ND

	St. 6
	100%
	ND
	80.0%
	20.0%
	ND
	100%
	
	100%
	ND
	95.7%
	4.3%
	ND
	100%

	St. 7
	100%
	ND
	81.8%
	18.2%
	ND
	100%
	
	100%
	ND
	94.9%
	5.1%
	ND
	100%

	St. 8
	91.9%
	8.9%
	100%
	ND
	ND
	ND
	
	99.9%
	0.1%
	100%
	ND
	ND
	ND

	Mean ± SD
	97.8± 2.9%
	2.2 ± 2.9%
	64.0 ± 33.0%
	36.0 ± 33.0%
	16.7 ± 40.8%
	83.3 ± 40.8%
	
	99.3 ± 1.0%
	0.7 ± 1.0%
	83.0 ± 34.4%
	17.0 ± 34.4%
	16.7 ± 40.8%
	83.3 ± 40.8%


Note: ND = Not detected.

Table S11 Relative composition of microplastic polymer types by particle count in sediment samples collected from eight stations in Tokyo Bay during October–November 2023.
	Polymer type
	St. 1
	St. 2
	St. 3
	St. 4
	St. 5
	St. 6
	St. 7
	St. 8
	Mean ± SD
	Num. of
detected
stations

	ABS
	ND
	ND
	ND
	ND
	ND
	1.6%
	ND
	ND
	0.2 ± 0.6%
	1

	alkyd
	ND
	ND
	ND
	2.5%
	3.4%
	1.6%
	1.5%
	3.2%
	1.5 ± 1.4%
	5

	epoxy
	ND
	ND
	ND
	ND
	ND
	ND
	1.5%
	ND
	0.2 ± 0.5%
	1

	PA
	ND
	ND
	8.2%
	1.3%
	1.1%
	1.6%
	ND
	1.6%
	1.7 ± 2.7%
	5

	PE
	18.2%
	73.2%
	36.7%
	12.5%
	33.3%
	42.9%
	42.6%
	64.5%
	40.5 ± 20.7%
	8

	PET
	27.3%
	9.8%
	2.0%
	ND
	1.1%
	7.9%
	13.2%
	1.6%
	7.9 ± 9.2%
	7

	PMMA
	2.3%
	2.4%
	4.1%
	1.3%
	1.1%
	17.5%
	26.5%
	ND
	6.9 ± 9.7%
	7

	PP
	50.0%
	12.2%
	42.9%
	72.5%
	52.9%
	22.2%
	13.2%
	29.0%
	36.9 ± 21.3%
	8

	PS
	ND
	2.4%
	6.1%
	8.8%
	4.6%
	4.8%
	ND
	ND
	3.3 ± 3.3%
	5

	PU
	2.3%
	ND
	ND
	ND
	1.1%
	ND
	1.5%
	ND
	0.6 ± 0.9%
	3

	PVC
	ND
	ND
	ND
	1.3%
	1.1%
	ND
	ND
	ND
	0.3 ± 0.6%
	2


Note: ND = Not detected.

Table S12 Relative composition of microplastic polymer types by estimated mass in sediment samples collected from eight stations in Tokyo Bay during October–November 2023.
	Polymer type
	St. 1
	St. 2
	St. 3
	St. 4
	St. 5
	St. 6
	St. 7
	St. 8
	Mean ± SD
	Num. of
detected
stations

	ABS
	ND
	ND
	ND
	ND
	ND
	1.0%
	ND
	ND
	0.1 ± 0.3%
	1

	alkyd
	ND
	ND
	ND
	7.6%
	70.8%
	2.5%
	5.5%
	3.8%
	11.3 ± 24.2%
	5

	epoxy
	ND
	ND
	ND
	ND
	ND
	ND
	13.7%
	ND
	1.7 ± 4.9%
	1

	PA
	ND
	ND
	11.6%
	0.9%
	0.6%
	1.0%
	ND
	0.02%
	1.8 ± 4.0%
	5

	PE
	3.8%
	80.9%
	31.0%
	4.0%
	8.6%
	59.1%
	21.5%
	65.8%
	34.3 ± 30.4%
	8

	PET
	88.1%
	8.2%
	12.4%
	ND
	0.04%
	12.1%
	16.3%
	1.7%
	17.3 ± 29.3%
	7

	PMMA
	1.3%
	3.0%
	3.5%
	0.1%
	0.6%
	9.3%
	36.7%
	ND
	6.8 ± 12.5%
	7

	PP
	6.6%
	7.4%
	34.8%
	85.8%
	16.1%
	14.1%
	4.5%
	28.7%
	24.7 ± 26.9%
	8

	PS
	ND
	0.5%
	6.8%
	1.0%
	1.4%
	1.0%
	ND
	ND
	1.4 ± 2.3%
	5

	PU
	0.2%
	ND
	ND
	ND
	0.3%
	ND
	1.7%
	ND
	0.3 ± 0.6%
	3

	PVC
	ND
	ND
	ND
	0.5%
	1.7%
	ND
	ND
	ND
	0.3 ± 0.6%
	2


Note: ND = Not detected.
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