Suppl. Table 1: Initial weight of desiccants resulted in different relative humidity inside the polystyrol box.
	Desiccant
	Initial weight
	approx. reached relative humidity

	sat. Potassium chloride
	33g/100 mL Aquadest.
	85%

	Lithium chloride
	23 g/ 100 mL Aquadest.
30 g/ 100 mL Aquadest.
[bookmark: _GoBack]40 g/ 100 mL Aquadest.
50 g/ 100 mL Aquadest.
	69%
57%
37%
31%

	freshly activated Silica gel
	100 g
	10%



