Comprehensive Approach Integrating Water Quality Index and Toxic Element Analysis for Environmental and Health Risk Assessment Enhanced by Simulation Techniques

Table S1. The results of the three samples used with mean and stand deviation values 
	Metals
	S1 (mg/L)
	S2 (mg/L)
	S3 (mg/L)
	Mean (mg/L)
	STD (mg/L)

	Mn
	0.002
	1.71
	0.422
	0.7113
	0.8321

	Fe
	0.002
	0.62
	0.152
	0.258
	0.3372

	Zn
	0.003
	0.88
	0.081
	0.3213
	0.4807

	Cu
	0.002
	0.16
	0.049
	0.0703
	0.0866



Table S2. The accuracy is determined by comparing the concentrations of the certified reference material to the known values.
	Metals
	 Mean (measured) (mg/L)
	CRM Value (mg/L)
	 Recovery (%)

	Mn
	0.422
	0.4
	105.5

	Fe
	0.152
	0.15
	101.3

	Zn
	0.081
	0.08
	101.3

	Cu
	0.049
	0.05
	98



Table S3. working standards, along with metal correlation coefficients.

	Metal
	Operational/working
standards
	Equation of calibration
	R2
	Sample. No

	Cu
	0.25, 1, 2.5, 5, 7.5
	y = 0.0215x−0.0039
	0.999
	1

	Fe
	0.05, 1, 2.5, 5, 7.5, 10
	y = 0.001x + 0.0009
	0.999
	2

	Zn
	0.5, 1, 1.5, 2.5, 3
	y = 0.0791x + 0.0019
	0.999
	3

	Mn
	0.05, 1, 2.5, 5, 7.5, 10
	y = 0.0025x + 0.0018
	0.999
	4



Table S4. The instrument's working conditions

	Metal
	Type of flame
	Wave length
(nm)
	Current of lamp
(mA)
	Slit width
(nm)

	Cu
	(Air/acetylene)
	324.5
	1.5
	1

	Fe
	
	248.3
	7.0
	2

	Zn
	
	213.9
	2.0
	3

	Mn
	
	294.9
	3
	4




Table S5. The parameters for the calculation of HQ, HI, and CR
	HM
	Cu
	Fe
	Mn
	Zn

	RfD Oral(mg/kg/day)
	0.04
	0.7
	0.024
	0.3

	ABS
	0.3
	0.2
	0.04
	0.2

	Rfd Dermal (mg/kg/day)
	0.012
	0.14
	0.00096
	0.06

	Kp
	0.001
	0.001
	0.001
	0.0006

	Si 
	3
	0.3
	0.05
	1

	ET Adult (h/day)
	0.58
	0.58
	0.58
	0.58

	ET Child (h/day)
	1
	1
	1
	1

	SA Adult (cm2)
	18000
	18000
	18000
	18000

	SA Child (cm2)
	6600
	6600
	6600
	6600

	CF (L/cm3)
	0.001
	0.001
	0.001
	0.001

	IR Adult (L/day)
	2.2
	2.2
	2.2
	2.2

	IR Child (L/day)
	1.8
	1.8
	1.8
	1.8

	EF (day/year)
	350
	350
	350
	350

	ED Adult (year)
	70
	70
	70
	70

	ED Child (year)
	6
	6
	6
	6

	BW Adult (kg)
	70
	70
	70
	70

	BW Child (kg)
	15
	15
	15
	15

	AT Adult (day)
	25550
	25550
	25550
	25550

	AT Child (day)
	2190
	2190
	2190
	2190

	Background (µg/g)
	30
	15000
	500
	100

	Tr
	5
	1
	1
	1




Table S6. The saturation index (SI) values of different minerals extracted from PHREEQC model
	Samples
	Anhydrite
	Calcite
	Dolomite
	Gypsum
	Halite
	CO2(g)

	1
	-1.1
	0.27
	0.13
	-0.87
	-4.32
	-2.84

	2
	-2.57
	0.1
	0.14
	-2.32
	-5.76
	-2.08

	3
	-2.33
	0.16
	0.81
	-2.1
	-5.82
	-2.57

	4
	-3.02
	0.7
	1.79
	-2.79
	-7.24
	-2.73

	5
	-3.13
	-0.99
	-1.59
	-2.91
	-6.99
	-1.08

	6
	-2.33
	0.03
	0.31
	-2.09
	-5.42
	-1.77

	7
	-3.07
	1.22
	2.18
	-2.83
	-7.15
	-2.42

	8
	-1.71
	0.74
	1.38
	-1.48
	-6.58
	-2.08

	9
	-2.19
	-0.33
	-0.74
	-1.97
	-7.22
	-2.45

	10
	-3.31
	-0.3
	-0.64
	-3.09
	-5.77
	-1.96

	11
	-2.43
	0.26
	0.4
	-2.21
	-7.86
	-2.74

	12
	-2.11
	-0.23
	-0.65
	-1.89
	-7.36
	-2.42

	13
	-2.07
	0.67
	1.33
	-1.83
	-5.57
	-2.8

	14
	-2.78
	1.14
	2.46
	-2.55
	-5.82
	-2.47

	15
	-3.14
	0.67
	1.81
	-2.91
	-7.03
	-2.45

	16
	-3.07
	0.24
	1.18
	-2.84
	-5.92
	-2.62

	17
	-5.23
	0.74
	1.57
	-5.01
	-7.03
	-2.36

	18
	-5.78
	0.32
	1.28
	-5.55
	-6.49
	-2.77

	19
	-5.62
	-0.1
	0.41
	-5.4
	-6.76
	-2.6

	20
	-4.12
	0.22
	0.98
	-3.9
	-6.4
	-2.65

	21
	-5.93
	0.13
	1.04
	-5.71
	-6.67
	-2.81

	22
	-4.23
	-0.69
	-0.22
	-4.01
	-6.4
	-2.1

	23
	-3.66
	-0.77
	-0.75
	-3.44
	-5.96
	-2.49

	24
	-1.65
	0.85
	1.65
	-1.42
	-6.52
	-2.2

	25
	-2.19
	-0.26
	-0.35
	-1.98
	-7.17
	-2.49

	26
	-1.99
	-0.42
	-1.07
	-1.75
	-7.22
	-2.37

	27
	-2.29
	0.7
	1.44
	-2.06
	-7.32
	-2.47

	28
	-2.72
	-0.24
	-0.49
	-2.48
	-7.94
	-2.61

	29
	-1.49
	0.57
	1.13
	-1.26
	-5.98
	-2.07

	30
	-2.63
	-0.1
	-0.35
	-2.41
	-8.05
	-2.75

	31
	-2.66
	-0.19
	-0.58
	-2.44
	-8
	-2.64

	32
	-2.39
	-0.57
	-1.23
	-2.17
	-7.81
	-2.25

	33
	-1.87
	0.36
	0.78
	-1.64
	-6.06
	-2.23

	34
	-1.55
	0.32
	0.77
	-1.33
	-5.97
	-2.21

	35
	-1.65
	0.37
	0.8
	-1.42
	-6.44
	-2.02

	36
	-1.74
	0.14
	0.04
	-1.51
	-5.94
	-2.1

	37
	-1.76
	0.76
	1.47
	-1.53
	-6.11
	-2.44

	38
	-1.93
	0.14
	0.2
	-1.72
	-6.81
	-1.72

	39
	-1.97
	0.6
	1.3
	-1.73
	-6.44
	-1.97

	40
	-1.3
	0.02
	-0.06
	-1.07
	-5.52
	-1.58

	41
	-2.36
	-0.42
	-1.04
	-2.13
	-7.82
	-2.34

	42
	-2
	-0.4
	-0.9
	-1.78
	-7.26
	-2.36

	43
	-1.79
	0.56
	1.09
	-1.57
	-6.59
	-1.88

	44
	-2.13
	0.73
	1.44
	-1.92
	-6.68
	-2

	45
	-2.41
	0.79
	1.42
	-2.16
	-6.99
	-2.17

	46
	-1.53
	0.67
	1.24
	-1.29
	-5.8
	-2.1

	47
	-1.38
	0.92
	1.74
	-1.17
	-5.64
	-1.63

	48
	-1.82
	0.53
	0.97
	-1.59
	-6.78
	-1.67

	49
	-1.47
	1.04
	1.72
	-1.23
	-5.86
	-1.68

	50
	-1.55
	0.81
	1.38
	-1.32
	-5.91
	-2.05

	51
	-1.98
	0.81
	1.84
	-1.75
	-5.91
	-2.14

	52
	-1.65
	0.72
	1.27
	-1.42
	-6.33
	-1.94

	53
	-1.84
	1.09
	2.15
	-1.68
	-6.6
	-1.91

	54
	-1.65
	0.79
	1.51
	-1.42
	-6.33
	-2.05

	55
	-1.78
	1.32
	2.42
	-1.57
	-6.36
	-2.34

	56
	-1.76
	0.65
	1
	-1.55
	-6.39
	-1.97

	57
	-1.58
	0.82
	1.24
	-1.36
	-6.46
	-2.04

	58
	-1.48
	0.81
	1.55
	-1.26
	-5.87
	-2.13

	59
	-2.25
	0.2
	0.26
	-2.02
	-7.09
	-1.81

	60
	-0.62
	0.93
	1.49
	-0.39
	-4.84
	-1.93

	61
	-1.69
	0.56
	0.85
	-1.47
	-6.3
	-2.21

	62
	-1.07
	0.95
	1.52
	-0.85
	-5.33
	-2.13

	63
	-1.52
	0.9
	1.61
	-1.32
	-6.35
	-2.04

	64
	-2.03
	0.7
	1.38
	-1.81
	-6.6
	-2.06

	65
	-2.56
	0.1
	-0.02
	-2.35
	-7.95
	-2.59

	66
	-1.45
	0.36
	0.5
	-1.22
	-6.1
	-2.09

	67
	-0.95
	1.03
	1.96
	-0.74
	-4.16
	-2.11

	68
	-1.39
	0.77
	1.35
	-1.18
	-6.01
	-2.11

	69
	-1.26
	0.72
	1.09
	-1.03
	-5.61
	-1.39




Table S7. The HQ dermal values in both child and adult
	Samples
	HQCu
(dermal&adult)
	HQCu
(dermal&child)
	HQFe
(dermal&adult)
	HQFe
(dermal&child)
	HQMn
(dermal&adult)
	HQMn
(dermal&child)
	HQZn
(dermal&adult)
	
HQZn
(dermal&child)

	1
	1.9E-03
	5.6E-03
	1.3E-04
	3.9E-04
	7.4E-04
	2.2E-03
	7.2E-05
	2.1E-04

	2
	8.3E-04
	2.5E-03
	1.9E-04
	5.7E-04
	3.0E-03
	8.8E-03
	7.2E-05
	2.1E-04

	3
	1.2E-04
	3.5E-04
	2.1E-04
	6.3E-04
	6.0E-03
	1.8E-02
	8.6E-05
	2.5E-04

	4
	1.2E-03
	3.5E-03
	7.2E-05
	2.1E-04
	7.6E-03
	2.2E-02
	5.7E-05
	1.7E-04

	5
	6.0E-04
	1.8E-03
	1.8E-04
	5.4E-04
	7.4E-04
	2.2E-03
	1.1E-04
	3.4E-04

	6
	1.2E-04
	3.5E-04
	2.1E-04
	6.3E-04
	6.0E-03
	1.8E-02
	8.6E-05
	2.5E-04

	7
	2.4E-04
	7.0E-04
	2.3E-04
	6.9E-04
	3.0E-03
	8.8E-03
	5.7E-05
	1.7E-04

	8
	3.6E-04
	1.1E-03
	1.5E-04
	4.5E-04
	3.0E-03
	8.8E-03
	7.2E-05
	2.1E-04

	9
	7.2E-04
	2.1E-03
	9.2E-05
	2.7E-04
	3.0E-04
	8.8E-04
	2.9E-05
	8.4E-05

	10
	1.2E-03
	3.5E-03
	5.3E-04
	1.6E-03
	7.4E-03
	2.2E-02
	8.6E-05
	2.5E-04

	11
	2.4E-04
	7.0E-04
	1.8E-04
	5.4E-04
	1.2E-03
	3.5E-03
	7.2E-05
	2.1E-04

	12
	1.5E-03
	4.6E-03
	1.3E-04
	3.9E-04
	6.0E-04
	1.8E-03
	7.2E-05
	2.1E-04

	13
	1.1E-03
	3.2E-03
	1.7E-04
	5.1E-04
	1.2E-03
	3.5E-03
	4.3E-05
	1.3E-04

	14
	1.2E-04
	3.5E-04
	1.1E-04
	3.3E-04
	3.0E-03
	8.8E-03
	1.1E-05
	3.4E-05

	15
	4.8E-04
	1.4E-03
	3.2E-04
	9.3E-04
	5.2E-02
	1.5E-01
	8.6E-05
	2.5E-04

	16
	6.0E-04
	1.8E-03
	3.8E-04
	1.1E-03
	1.4E-01
	4.2E-01
	1.3E-04
	3.8E-04

	17
	3.6E-04
	1.1E-03
	3.4E-04
	9.9E-04
	1.3E-01
	3.9E-01
	1.0E-04
	3.0E-04

	18
	1.2E-03
	3.5E-03
	6.3E-04
	1.9E-03
	1.4E-01
	4.1E-01
	1.1E-04
	3.4E-04

	19
	3.6E-04
	1.1E-03
	3.1E-04
	9.0E-04
	6.9E-02
	2.0E-01
	1.6E-04
	4.6E-04

	20
	2.4E-05
	7.0E-05
	1.2E-04
	3.6E-04
	1.2E-01
	3.4E-01
	1.1E-04
	3.4E-04

	21
	6.0E-04
	1.8E-03
	3.8E-04
	1.1E-03
	1.4E-01
	4.2E-01
	1.3E-04
	3.8E-04

	22
	1.2E-03
	3.5E-03
	6.3E-04
	1.9E-03
	1.4E-01
	4.1E-01
	1.1E-04
	3.4E-04

	23
	4.2E-04
	1.2E-03
	4.8E-04
	1.4E-03
	1.0E-02
	3.0E-02
	2.4E-04
	7.1E-04

	24
	1.1E-04
	3.2E-04
	3.1E-06
	9.0E-06
	7.4E-04
	2.2E-03
	1.4E-05
	4.2E-05

	25
	7.9E-04
	2.3E-03
	2.7E-04
	8.0E-04
	7.0E-02
	2.1E-01
	2.3E-05
	6.8E-05

	26
	6.6E-04
	1.9E-03
	2.2E-04
	6.5E-04
	1.1E-02
	3.4E-02
	3.7E-05
	1.1E-04

	27
	6.1E-04
	1.8E-03
	2.6E-04
	7.5E-04
	3.7E-03
	1.1E-02
	1.3E-05
	3.8E-05

	28
	6.3E-04
	1.9E-03
	3.2E-04
	9.4E-04
	7.7E-03
	2.3E-02
	6.1E-04
	1.8E-03

	29
	6.2E-04
	1.8E-03
	1.9E-04
	5.5E-04
	7.8E-02
	2.3E-01
	8.6E-06
	2.5E-05

	30
	1.4E-04
	4.2E-04
	8.7E-05
	2.6E-04
	1.2E-01
	3.6E-01
	7.2E-06
	2.1E-05

	31
	6.1E-04
	1.8E-03
	2.3E-04
	6.9E-04
	1.4E-01
	4.0E-01
	1.1E-05
	3.4E-05

	32
	6.4E-04
	1.9E-03
	1.7E-04
	4.9E-04
	1.3E-02
	3.9E-02
	5.1E-05
	1.5E-04

	33
	6.0E-05
	1.8E-04
	6.1E-06
	1.8E-05
	1.5E-03
	4.4E-03
	1.1E-05
	3.4E-05

	34
	4.2E-04
	1.2E-03
	2.1E-04
	6.1E-04
	2.2E-03
	6.6E-03
	1.9E-05
	5.5E-05

	35
	5.7E-04
	1.7E-03
	2.0E-04
	5.9E-04
	1.3E-02
	3.9E-02
	5.1E-05
	1.5E-04

	36
	2.4E-04
	7.0E-04
	2.6E-04
	7.5E-04
	6.7E-02
	2.0E-01
	1.7E-04
	5.1E-04

	37
	6.0E-05
	1.8E-04
	7.2E-06
	2.1E-05
	8.9E-04
	2.6E-03
	4.3E-06
	1.3E-05

	38
	7.2E-05
	2.1E-04
	2.7E-04
	7.8E-04
	6.1E-02
	1.8E-01
	1.0E-04
	3.0E-04

	39
	2.4E-04
	7.0E-04
	2.3E-04
	6.9E-04
	1.0E-01
	3.1E-01
	0.0E+00
	0.0E+00

	40
	1.2E-04
	3.5E-04
	5.0E-04
	1.5E-03
	9.5E-02
	2.8E-01
	7.2E-05
	2.1E-04

	41
	3.6E-04
	1.1E-03
	2.1E-04
	6.3E-04
	1.2E-03
	3.5E-03
	4.3E-05
	1.3E-04

	42
	3.6E-04
	1.1E-03
	1.4E-04
	4.2E-04
	3.0E-03
	8.8E-03
	1.3E-03
	3.7E-03

	43
	3.3E-04
	9.8E-04
	3.2E-04
	9.4E-04
	1.9E-03
	5.7E-03
	1.9E-05
	5.5E-05

	44
	1.9E-03
	5.6E-03
	1.0E-06
	3.0E-06
	6.3E-02
	1.9E-01
	7.2E-05
	2.1E-04

	45
	8.3E-04
	2.5E-03
	2.0E-07
	6.0E-07
	1.0E-01
	3.0E-01
	7.2E-05
	2.1E-04

	46
	1.2E-04
	3.5E-04
	3.1E-06
	9.0E-06
	8.9E-02
	2.6E-01
	8.6E-05
	2.5E-04

	47
	1.2E-03
	3.5E-03
	1.0E-06
	3.0E-06
	1.9E-01
	5.6E-01
	5.7E-05
	1.7E-04

	48
	6.0E-04
	1.8E-03
	5.1E-06
	1.5E-05
	1.6E-01
	4.8E-01
	1.1E-04
	3.4E-04

	49
	1.2E-04
	3.5E-04
	2.0E-06
	6.0E-06
	2.5E-01
	7.5E-01
	8.6E-05
	2.5E-04

	50
	2.4E-04
	7.0E-04
	1.0E-06
	3.0E-06
	1.4E-01
	4.2E-01
	5.7E-05
	1.7E-04

	51
	3.6E-04
	1.1E-03
	3.1E-06
	9.0E-06
	9.0E-02
	2.7E-01
	7.2E-05
	2.1E-04

	52
	7.2E-04
	2.1E-03
	1.0E-06
	3.0E-06
	1.2E-01
	3.5E-01
	2.9E-05
	8.4E-05

	53
	1.2E-03
	3.5E-03
	5.1E-06
	1.5E-05
	1.6E-01
	4.8E-01
	8.6E-05
	2.5E-04

	54
	2.4E-04
	7.0E-04
	6.1E-06
	1.8E-05
	8.6E-02
	2.5E-01
	7.2E-05
	2.1E-04

	55
	1.5E-03
	4.6E-03
	1.0E-06
	3.0E-06
	2.4E-02
	7.1E-02
	7.2E-05
	2.1E-04

	56
	1.1E-03
	3.2E-03
	2.0E-06
	6.0E-06
	4.8E-02
	1.4E-01
	4.3E-05
	1.3E-04

	57
	1.2E-04
	3.5E-04
	3.1E-06
	9.0E-06
	5.3E-02
	1.6E-01
	1.1E-05
	3.4E-05

	58
	4.8E-04
	1.4E-03
	2.0E-06
	6.0E-06
	1.6E-01
	4.7E-01
	8.6E-05
	2.5E-04

	59
	6.0E-04
	1.8E-03
	4.1E-06
	1.2E-05
	6.9E-03
	2.0E-02
	1.3E-04
	3.8E-04

	60
	3.6E-04
	1.1E-03
	4.1E-06
	1.2E-05
	8.0E-02
	2.4E-01
	1.0E-04
	3.0E-04

	61
	1.2E-03
	3.5E-03
	2.0E-06
	6.0E-06
	4.7E-02
	1.4E-01
	1.1E-04
	3.4E-04

	62
	3.6E-04
	1.1E-03
	3.1E-06
	9.0E-06
	2.2E-01
	6.5E-01
	1.6E-04
	4.6E-04

	63
	2.4E-05
	7.0E-05
	1.0E-06
	3.0E-06
	9.8E-02
	2.9E-01
	1.1E-04
	3.4E-04

	64
	6.0E-04
	1.8E-03
	1.0E-06
	3.0E-06
	1.3E-02
	3.8E-02
	1.3E-04
	3.8E-04

	65
	1.2E-03
	3.5E-03
	1.0E-06
	3.0E-06
	6.1E-02
	1.8E-01
	1.1E-04
	3.4E-04

	66
	4.2E-04
	1.2E-03
	1.0E-06
	3.0E-06
	4.3E-02
	1.3E-01
	2.4E-04
	7.1E-04

	67
	1.1E-04
	3.2E-04
	1.0E-06
	3.0E-06
	9.5E-02
	2.8E-01
	1.4E-05
	4.2E-05

	68
	1.2E-04
	3.5E-04
	1.0E-06
	3.0E-06
	7.0E-03
	2.1E-02
	1.1E-05
	3.4E-05

	69
	4.8E-04
	1.4E-03
	1.0E-06
	3.0E-06
	2.1E-02
	6.1E-02
	8.6E-05
	2.5E-04

	Min
	2.4E-05
	7.0E-05
	2.0E-07
	6.0E-07
	3.0E-04
	8.8E-04
	0.00E+00
	0.00E+00

	Max
	1.9E-03
	5.6E-03
	6.3E-04
	1.9E-03
	2.5E-01
	7.5E-01
	1.3E-03
	3.7E-03

	Average
	5.8E-04
	1.7E-03
	1.5E-04
	4.6E-04
	6.3E-02
	1.9E-01
	1.1E-04
	3.4E-04





Table S8. The HQ oral values in both child and adult
	Samples
	HQCu 
(oral&adult)
	HQCu 
(oral&child)
	HQFe 
(oral&adult)
	HQFe 
(oral&child)
	HQMn
 (oral&adult)
	HQMn
 (oral&child)
	HQZn 
(oral&adult)
	HQZn 
(oral&child)

	1
	1.2E-01
	4.6E-01
	5.6E-03
	2.1E-02
	6.3E-03
	2.4E-02
	5.0E-03
	1.9E-02

	2
	5.3E-02
	2.0E-01
	8.2E-03
	3.1E-02
	2.5E-02
	9.6E-02
	5.0E-03
	1.9E-02

	3
	7.5E-03
	2.9E-02
	9.0E-03
	3.5E-02
	5.0E-02
	1.9E-01
	6.0E-03
	2.3E-02

	4
	7.5E-02
	2.9E-01
	3.0E-03
	1.2E-02
	6.4E-02
	2.4E-01
	4.0E-03
	1.5E-02

	5
	3.8E-02
	1.4E-01
	7.7E-03
	3.0E-02
	6.3E-03
	2.4E-02
	8.0E-03
	3.1E-02

	6
	7.5E-03
	2.9E-02
	9.0E-03
	3.5E-02
	5.0E-02
	1.9E-01
	6.0E-03
	2.3E-02

	7
	1.5E-02
	5.8E-02
	9.9E-03
	3.8E-02
	2.5E-02
	9.6E-02
	4.0E-03
	1.5E-02

	8
	2.3E-02
	8.6E-02
	6.5E-03
	2.5E-02
	2.5E-02
	9.6E-02
	5.0E-03
	1.9E-02

	9
	4.5E-02
	1.7E-01
	3.9E-03
	1.5E-02
	2.5E-03
	9.6E-03
	2.0E-03
	7.7E-03

	10
	7.5E-02
	2.9E-01
	2.2E-02
	8.5E-02
	6.3E-02
	2.4E-01
	6.0E-03
	2.3E-02

	11
	1.5E-02
	5.8E-02
	7.7E-03
	3.0E-02
	1.0E-02
	3.8E-02
	5.0E-03
	1.9E-02

	12
	9.8E-02
	3.7E-01
	5.6E-03
	2.1E-02
	5.0E-03
	1.9E-02
	5.0E-03
	1.9E-02

	13
	6.8E-02
	2.6E-01
	7.3E-03
	2.8E-02
	1.0E-02
	3.8E-02
	3.0E-03
	1.2E-02

	14
	7.5E-03
	2.9E-02
	4.7E-03
	1.8E-02
	2.5E-02
	9.6E-02
	8.0E-04
	3.1E-03

	15
	3.0E-02
	1.2E-01
	1.3E-02
	5.1E-02
	4.4E-01
	1.7E+00
	6.0E-03
	2.3E-02

	16
	3.8E-02
	1.4E-01
	1.6E-02
	6.1E-02
	1.2E+00
	4.6E+00
	9.0E-03
	3.5E-02

	17
	2.3E-02
	8.6E-02
	1.4E-02
	5.4E-02
	1.1E+00
	4.2E+00
	7.0E-03
	2.7E-02

	18
	7.5E-02
	2.9E-01
	2.7E-02
	1.0E-01
	1.2E+00
	4.5E+00
	8.0E-03
	3.1E-02

	19
	2.3E-02
	8.6E-02
	1.3E-02
	4.9E-02
	5.8E-01
	2.2E+00
	1.1E-02
	4.2E-02

	20
	1.5E-03
	5.8E-03
	5.2E-03
	2.0E-02
	9.8E-01
	3.7E+00
	8.0E-03
	3.1E-02

	21
	3.8E-02
	1.4E-01
	1.6E-02
	6.1E-02
	1.2E+00
	4.6E+00
	9.0E-03
	3.5E-02

	22
	7.5E-02
	2.9E-01
	2.7E-02
	1.0E-01
	1.2E+00
	4.5E+00
	8.0E-03
	3.1E-02

	23
	2.6E-02
	1.0E-01
	2.0E-02
	7.7E-02
	8.5E-02
	3.3E-01
	1.7E-02
	6.4E-02

	24
	6.8E-03
	2.6E-02
	1.3E-04
	4.9E-04
	6.3E-03
	2.4E-02
	1.0E-03
	3.8E-03

	25
	5.0E-02
	1.9E-01
	1.1E-02
	4.4E-02
	5.9E-01
	2.3E+00
	1.6E-03
	6.1E-03

	26
	4.1E-02
	1.6E-01
	9.3E-03
	3.5E-02
	9.7E-02
	3.7E-01
	2.6E-03
	1.0E-02

	27
	3.8E-02
	1.5E-01
	1.1E-02
	4.1E-02
	3.1E-02
	1.2E-01
	9.0E-04
	3.5E-03

	28
	4.0E-02
	1.5E-01
	1.3E-02
	5.1E-02
	6.5E-02
	2.5E-01
	4.3E-02
	1.6E-01

	29
	3.9E-02
	1.5E-01
	7.8E-03
	3.0E-02
	6.6E-01
	2.5E+00
	6.0E-04
	2.3E-03

	30
	9.0E-03
	3.5E-02
	3.7E-03
	1.4E-02
	1.0E+00
	3.9E+00
	5.0E-04
	1.9E-03

	31
	3.8E-02
	1.5E-01
	9.8E-03
	3.7E-02
	1.2E+00
	4.4E+00
	8.0E-04
	3.1E-03

	32
	4.1E-02
	1.6E-01
	7.0E-03
	2.7E-02
	1.1E-01
	4.2E-01
	3.6E-03
	1.4E-02

	33
	3.8E-03
	1.4E-02
	2.6E-04
	9.9E-04
	1.3E-02
	4.8E-02
	8.0E-04
	3.1E-03

	34
	2.6E-02
	1.0E-01
	8.7E-03
	3.3E-02
	1.9E-02
	7.2E-02
	1.3E-03
	5.0E-03

	35
	3.6E-02
	1.4E-01
	8.5E-03
	3.2E-02
	1.1E-01
	4.2E-01
	3.6E-03
	1.4E-02

	36
	1.5E-02
	5.8E-02
	1.1E-02
	4.1E-02
	5.7E-01
	2.2E+00
	1.2E-02
	4.6E-02

	37
	3.8E-03
	1.4E-02
	3.0E-04
	1.2E-03
	7.5E-03
	2.9E-02
	3.0E-04
	1.2E-03

	38
	4.5E-03
	1.7E-02
	1.1E-02
	4.3E-02
	5.1E-01
	2.0E+00
	7.0E-03
	2.7E-02

	39
	1.5E-02
	5.8E-02
	9.9E-03
	3.8E-02
	8.8E-01
	3.4E+00
	0.0E+00
	0.0E+00

	40
	7.5E-03
	2.9E-02
	2.1E-02
	8.1E-02
	8.0E-01
	3.1E+00
	5.0E-03
	1.9E-02

	41
	2.3E-02
	8.6E-02
	9.0E-03
	3.5E-02
	1.0E-02
	3.8E-02
	3.0E-03
	1.2E-02

	42
	2.3E-02
	8.6E-02
	6.0E-03
	2.3E-02
	2.5E-02
	9.6E-02
	8.8E-02
	3.4E-01

	43
	2.1E-02
	8.1E-02
	1.3E-02
	5.1E-02
	1.6E-02
	6.2E-02
	1.3E-03
	5.0E-03

	44
	1.2E-01
	4.6E-01
	4.3E-05
	1.6E-04
	5.3E-01
	2.0E+00
	5.0E-03
	1.9E-02

	45
	5.3E-02
	2.0E-01
	8.6E-06
	3.3E-05
	8.5E-01
	3.2E+00
	5.0E-03
	1.9E-02

	46
	7.5E-03
	2.9E-02
	1.3E-04
	4.9E-04
	7.5E-01
	2.9E+00
	6.0E-03
	2.3E-02

	47
	7.5E-02
	2.9E-01
	4.3E-05
	1.6E-04
	1.6E+00
	6.1E+00
	4.0E-03
	1.5E-02

	48
	3.8E-02
	1.4E-01
	2.2E-04
	8.2E-04
	1.4E+00
	5.2E+00
	8.0E-03
	3.1E-02

	49
	7.5E-03
	2.9E-02
	8.6E-05
	3.3E-04
	2.1E+00
	8.2E+00
	6.0E-03
	2.3E-02

	50
	1.5E-02
	5.8E-02
	4.3E-05
	1.6E-04
	1.2E+00
	4.6E+00
	4.0E-03
	1.5E-02

	51
	2.3E-02
	8.6E-02
	1.3E-04
	4.9E-04
	7.6E-01
	2.9E+00
	5.0E-03
	1.9E-02

	52
	4.5E-02
	1.7E-01
	4.3E-05
	1.6E-04
	1.0E+00
	3.9E+00
	2.0E-03
	7.7E-03

	53
	7.5E-02
	2.9E-01
	2.2E-04
	8.2E-04
	1.4E+00
	5.2E+00
	6.0E-03
	2.3E-02

	54
	1.5E-02
	5.8E-02
	2.6E-04
	9.9E-04
	7.2E-01
	2.8E+00
	5.0E-03
	1.9E-02

	55
	9.8E-02
	3.7E-01
	4.3E-05
	1.6E-04
	2.0E-01
	7.8E-01
	5.0E-03
	1.9E-02

	56
	6.8E-02
	2.6E-01
	8.6E-05
	3.3E-04
	4.0E-01
	1.5E+00
	3.0E-03
	1.2E-02

	57
	7.5E-03
	2.9E-02
	1.3E-04
	4.9E-04
	4.4E-01
	1.7E+00
	8.0E-04
	3.1E-03

	58
	3.0E-02
	1.2E-01
	8.6E-05
	3.3E-04
	1.3E+00
	5.1E+00
	6.0E-03
	2.3E-02

	59
	3.8E-02
	1.4E-01
	1.7E-04
	6.6E-04
	5.8E-02
	2.2E-01
	9.0E-03
	3.5E-02

	60
	2.3E-02
	8.6E-02
	1.7E-04
	6.6E-04
	6.7E-01
	2.6E+00
	7.0E-03
	2.7E-02

	61
	7.5E-02
	2.9E-01
	8.6E-05
	3.3E-04
	3.9E-01
	1.5E+00
	8.0E-03
	3.1E-02

	62
	2.3E-02
	8.6E-02
	1.3E-04
	4.9E-04
	1.9E+00
	7.1E+00
	1.1E-02
	4.2E-02

	63
	1.5E-03
	5.8E-03
	4.3E-05
	1.6E-04
	8.3E-01
	3.2E+00
	8.0E-03
	3.1E-02

	64
	3.8E-02
	1.4E-01
	4.3E-05
	1.6E-04
	1.1E-01
	4.1E-01
	9.0E-03
	3.5E-02

	65
	7.5E-02
	2.9E-01
	4.3E-05
	1.6E-04
	5.1E-01
	2.0E+00
	8.0E-03
	3.1E-02

	66
	2.6E-02
	1.0E-01
	4.3E-05
	1.6E-04
	3.6E-01
	1.4E+00
	1.7E-02
	6.4E-02

	67
	6.8E-03
	2.6E-02
	4.3E-05
	1.6E-04
	8.0E-01
	3.0E+00
	1.0E-03
	3.8E-03

	68
	7.5E-03
	2.9E-02
	4.3E-05
	1.6E-04
	5.9E-02
	2.3E-01
	8.0E-04
	3.1E-03

	69
	3.0E-02
	1.2E-01
	4.3E-05
	1.6E-04
	1.7E-01
	6.6E-01
	6.0E-03
	2.3E-02

	Min
	1.5E-03
	5.8E-03
	8.6E-06
	3.3E-05
	2.5E-03
	9.6E-03
	0.0E+00
	0.0E+00

	Max
	1.2E-01
	4.6E-01
	2.7E-02
	1.0E-01
	2.1E+00
	8.2E+00
	8.8E-02
	3.4E-01

	Average
	3.7E-02
	1.4E-01
	6.5E-03
	2.5E-02
	5.3E-01
	2.0E+00
	8.0E-03
	3.1E-02



