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Table A1. Characteristic matrix for class assignation for constructions with household use based on the Characteristic Matrix form the Mexico City building code 2021 (Congreso de la Ciudad de Mexico 2021)

	Construction
Area m2
	Class

	1-50
	1

	50-85
	2

	85-150
	3

	150-250
	4

	250-450
	5

	450-650
	6

	> 650
	7



Table A2. Characteristic matrix for class assignation for constructions with household use that has been adapted to office, hotel, commerce, health care, education and communication uses based on the Characteristic Matrix form the Mexico City building code 2021 (Congreso de la Ciudad de Mexico 2021)

	Construction
Area m2
	Class

	1-50
	1

	50-85
	2

	85-150
	3

	150-250
	4

	250-450
	5

	450-650
	6

	> 650
	7



Table A3. Characteristic matrix for class assignation for constructions with office, hotel, commerce, health care, education, and communication use based on the Characteristic Matrix form the Mexico City building code 2021 (Congreso de la Ciudad de Mexico 2021)

	Number of levels
	Class

	1
	1

	1-2
	2

	2-5
	3

	5-10
	4

	10-15
	5

	15-25
	6

	> 25
	7



Table A4. Characteristic matrix for class assignation for constructions with industrial, warehousing and cultural use based on the Characteristic Matrix form the Mexico City building code 2021 (Congreso de la Ciudad de Mexico 2021)

	High (m)
	Class

	2.5
	1

	2.5-3.5
	2

	3.5-5
	3

	5-6
	4

	6-8
	5

	8-10
	6

	> 10
	7



Table A5. Characteristic matrix for class assignation for constructions with sport use based on the Characteristic Matrix form the Mexico City building code 2021 (Congreso de la Ciudad de Mexico 2021)

	High (m)
	Class

	3
	1

	3-6
	2

	6-12
	3

	12-20
	4

	20-25
	5

	25-35
	6

	> 35
	7



