Table S1. List of ASTM methods and descriptions for the ultimate and proximate analyses of biomass.

	Fuel Property
	ASTM Method
	Method Description

	Proximate Analysis
	
	
	

	
	Moisture Content
	E871
	Moisture Analysis of Particulate Wood Fuels

	
	
	D3173
	Moisture in the Analysis Sample of Coal and Coke

	
	Volatile Matter
	E872
	Volatile Matter in the Analysis of Particulate Wood Fuels

	
	
	D3175
	Volatile Matter in the Analysis Sample of Coal and Coke

	
	Ash
	D1102
	Ash in Wood

	
	
	D3174
	Ash in the Analysis Sample of Coal and Coke

	
	
	E1755
	Standard Ash in Biomass

	
	Fixed Carbon
	E870
	Calculated from mass difference

	
	
	
	

	Ultimate Analysis
	
	
	

	
	Carbon
	E777
	Carbon and Hydrogen in the Analysis of 
Refuse-Derived Fuel

	
	Hydrogen
	E777
	Carbon and Hydrogen in the Analysis of 
Refuse-Derived Fuel

	
	Nitrogen
	E778
	Nitrogen in the Analysis of 
Refuse-Derived Fuel

	
	Sulfur
	E775
	Total Sulfur in the Analysis of 
Refuse-Derived Fuel

	
	Oxygen
	E870
	Calculated from mass difference


