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Table 1. Trampoline mechanistic specifications


















	


Table 2. Spring specifications (mean ± standard deviation) of 10 springs from one batch
 
	Nominal (mm)
	Spring Length (mm)
	Spring Diameter (mm)
	Wire thickness (mm)
	Elastic limit length (mm)
	Spring Constant (N.mm-1)

	140
	133.7 ± 0.5
	22.1 ± 0.1
	3.2
	213 ± 0.3
	8.09 ± 0.44

	180
	174.2 ± 0.3
	24.9 ± 0.1
	3.2
	298 ± 0.6
	4.13 ± 0.14

	220
	216.0 ± 0.6
	24.8 ± 0.1
	3.2
	422 ± 0.9
	2.75 ± 0.64
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[bookmark: _GoBack]Fig 1. Load length plot from the tensile test for the 180 mm spring. The elastic limit is depicted by * and ultimate tensile strength at the end of the curve. Elastic limit was identified using a piecewise based regression method [27]. The maximum spring extension for the spring when on a 4.27 m (14 ft) trampoline is shown by the dotted line. Data starts with an initial load of 50 N.
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