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	Plasma conditions: Tune Parameters

	RF Power
	1550 W

	RF Matching
	1.80 V

	Sample Depth
	10.0 mm

	Nebulizer Gas
	0.99 L/min

	Gas Switch
	Makeup Gas

	Makeup/Dilution Gas
	0.00 L/min

	Option Gas
	0.0 %

	Nebulizer Pump
	0.10 rps

	S/C Temp
	2 ºC

	Plasma Gas
	15.0 L/min

	Auxiliary Gas
	0.90 L/min

	Torch conditions: Hardware Settings

	Torch H
	0.1 mm

	Torch V
	0.2 mm



Table S2. Method detection limits for the analysed elements.
	Element
	DL (µg g-1)

	Mg
	0.125

	P
	1.25

	K
	3.875

	Ca
	12.5

	Mn
	0.004

	Fe
	0.06

	Cu
	0.042

	Zn
	0.075



