Description of Supplementary Files


File Name: Supplementary Movie 1
Description: ECL imaging of large electrode taken at 0.1 µm distance from the Ru@ITO emitting surface during a CV scanning in TPrA 180mM in 0.2M Phosphate Buffer (PB, pH 6.9). Potential 0-1.4 V vs. Ag/AgCl (3 M KCl), scan rate 100 mV s-1, exposure time 200 ms, and magnification 4x.
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File Name: Supplementary Movie 2
Description: ECL imaging of small electrode taken at 0.1 µm distance from the Ru@ITO emitting surface during a CV scanning in TPrA 180mM in 0.2M Phosphate Buffer (PB, pH 6.9). Potential 0-1.4 V vs. Ag/AgCl (3 M KCl), scan rate 100 mV s-1, exposure time: 200 ms, and magnification 4x.
