{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["平地","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"平地","index":0,"n_rows":12,"n_cols":18,"rows_kept":12,"merged":[[0,0,0,3],[0,6,0,10],[0,13,0,17],[2,0,3,0],[2,1,3,1],[2,2,3,2],[5,0,6,0],[5,1,6,1],[5,2,6,2],[7,0,8,0],[7,1,8,1],[7,2,8,2],[9,0,10,0],[9,1,10,1],[9,2,10,2]],"flags":["formulas_cached_only"]}
["Table 1. Material properties of model components",{"$nulls":5},"Table 2. Foot displacement and tissue stresses under static bilateral stance for insoles with varying Young’s moduli.",{"$nulls":6},"Table 3. Foot displacement and tissue stresses under forefoot contact phase of gait for insoles with varying Young’s moduli."]
["Components","Young’s modulus (MPa)","Poisson’s ratio","Element type",null,null,"Insole material（MPa）","foot displacement （mm）","medial process of the calcaneal tuberosity stress (MPa)","metatarsal stress (MPa)","plantar stress (MPa)",null,null,"Insole material（MPa）","foot displacement （mm）","medial process of the calcaneal tuberosity stress (MPa)","metatarsal stress (MPa)","plantar stress (MPa)"]
["Cartilage",1,0.42,"4-node linear",null,null,"EVA (100)",3.154,82.24,19.76,0.426,null,null,"EVA (100)",5.639,118.6,25.87,0.783]
[{"$nulls":3},"tetrahedrone",null,null,"PU (260)",3.111,81.51,19.72,0.418,null,null,"PU (260)",4.06,99.46,23.48,0.456]
["Soft tissue",1.15,0.49,"4-node tetrahedrone",null,null,"TPU (1000)",3.075,80.71,19.66,0.419,null,null,"TPU (1000)",3.281,87.81,21.43,0.41]
["Ligament",260,0,"2-node linear 3-D",null,null,"TPE (3000)",3.057,80.23,19.63,0.414,null,null,"TPE (3000)",3.06,84.45,20.79,0.408]
[{"$nulls":3},"trusse",null,null,"Plastic (5000)",3.051,80.06,19.62,0.411,null,null,"Plastic (5000)",3.012,83.68,20.66,0.405]
["Cortical bone",7300,0.3,"4-node linear",null,null,"Rigid (500000)",3.034,79.5,19.63,0.405,null,null,"Rigid (500000)",2.933,82.1,20.48,0.411]
[{"$nulls":3},"tetrahedrone"]
["Cancellous bone",100,0.3,"4-node linear"]
[{"$nulls":3},"tetrahedrone"]
["Ground",17000,0.1,"8-node linear bricke"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}