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Description automatically generated]
Supplementary file 3: Average overlapping area between images from consecutive flight paths. FP1 and FP2 are flight paths 1 and 2. X is the average mean distance between consecutive flight paths. W1 and W2 ate is the widths of parallel images and H the height of images. WO is the width of overlapping area between parallel images from consecutive flight paths. 
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