Table 1: Experimental phases and SCR operation schedule

	phases
	Run
	Day
	[bookmark: OLE_LINK595][bookmark: OLE_LINK596][bookmark: OLE_LINK593][bookmark: OLE_LINK594]Catechol inlet (mg/L)
	COD inlet
(mg/L)
	Flow rate (L/d)
	HRT
(h)
	OLR
kg COD/m3.d

	Reactor start-up
	0
	0-35
	630
	1183
	6.28
	15
	1.52

	[bookmark: _Hlk337754906]Effect of catechol concentration


	A
	35-47
	630
	1183
	6.28
	15
	1.52

	
	B
	48-80
	930
	1750
	6.28
	15
	2.21

	[bookmark: _Hlk336824262]
	C
	81-90
	1294
	2433
	6.28
	15
	3.17

	
	D
	[bookmark: OLE_LINK620][bookmark: OLE_LINK621]91-124
	1560
	2933
	[bookmark: OLE_LINK609][bookmark: OLE_LINK610][bookmark: OLE_LINK613]6.28
	15
	3.82

	Effect of HRT
	D
	91-124
	1560
	2933
	6.28
	15
	3.82

	
	E
	125-158
	1560
	2933
	10.67
	10
	5.38

	[bookmark: _Hlk336823759]
	F
	159-166
	1560
	2933
	25.12
	6
	7.82




