List of abbreviations 

Avg TC		average Transport Costs [Euro]
C crew		Crew costs [Euro]
C fixed		Fixed maintenance costs [Euro/m3]
C fuel		Fuel costs [Euro]
C maintenance	Maintenance costs [Euro]
C var		Variable costs of maintenance [Euro/KWh]
CF		Consumption Factor [kgCO2e/kg]
CS		Consumer surplus [Euro]
D		Demand (IWT volume) [tonnes]
D ports		port dues [Euro]
EC		Economic benefit [Euro]
EF		Emissions Factor [kgCO2e/tkm]
ETS		European Trading Scheme
FC		Fuel Consumption [kg]
FC idle		Fuel Consumption, when vessel not in movement (idle) [kg]
FD		Fairway Depth [m]
IWT		Inland Waterway Transport
k		proportionality constant, depending on size of vessel [unitless]
KPI		Key Performance Indicator
P		Price [Euro]
P installed	Power installed [KW]
PE		Price Elasticity [unitless]
S0		Scenario 0 (Scenario before bottleneck removal)
S1		Scenario 1(Schenario after bottleneck removal)
SB		Social benefit [Euro]
SL		Service level
SQ		Squat [m]
T idle		time, when vessel not in movement [hours]
TB		Total benefit [Euro]
TC		Transport Costs [Euro]
TD		Transport Duration [hours]
TE		Transport Emissions [kgCO2e]
TS		Transport Supply [tonnes]
TSav		Transport Emissions Savings [Euro]
UC		Underkeel Clearance [m]
VD		Vessel draft [m]
V		speed [km/h]
V critical	critical speed [m/s]
V current	speed of the current [m/s]
V power	speed at 85% of maximum power [m/s]


