	Mask Number
	Picture
	Manufacturer and model
	Mask type
	Shape
	Approval Standard
	Regulatory Status
	Exhalation Valve
	Tethering Devices
	Number of masks measured for weight and thickness*
	Average Thickness (mm)
	Average Weight (g/m2)

	1
	[image: ]
	3M K112
	FFP2
	duckbill
	EN149-2001
	Not on Appendix A
	Yes
	Headband straps
	1
	1.05
	223

	2
	[image: ]
	Guangzhou Kanglv 9501
	FFP2
	flatfold
	EN149-2001
	Not on Appendix A
	No
	Earloop straps
	1
	0.51
	111

	3
	[image: ]
	Aoxing KN95
	KN95
	flatfold
	GB2626-2006
	Appendix A
(FDA Authorized)
	No
	Earloop straps
	1
	0.85
	174

	4
	[image: ]
	aRUN Industrial Co N9
	KN95
	flatfold
	GB2626-2006
	Appendix A
(FDA Authorized)
	No
	Earloop straps
	1
	0.58
	127

	5
	[image: ]
	Graphene SNN70370B
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	Yes
	Earloop straps
	2
	0.7 ± 0.03
	162 ± 4

	[bookmark: _GoBack]6
	[image: ]
	HuaGang Communication Disposable Face Mask
	KN95
	flatfold
	GB2626-2006
	Formerly on Appendix A
	No
	Earloop straps
	1
	0.67
	166

	7
	[image: ]
	Jinan Vhold Co. VH95
	KN95
	flatfold
	GB2626-2006
	Formerly on Appendix A
	No
	Earloop straps
	5
	1.04 ± 0.07
	233 ± 12

	8
	[image: ]
	SNIPPET SNB9501
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	2
	0.82 ± 0.03
	198 ± 6

	9
	[image: ]
	Urance KN95
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	1
	0.56
	126

	10
	[image: ]
	Yimengshan 9201
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	2
	0.83 ± 0.02
	200 ± 1

	11
	[image: ]
	Yuxu 9901
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	1
	0.85
	189

	12
	[image: ]
	Unmarked batch #1
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	1
	0.75
	177

	13
	[image: ]
	Unmarked batch #2
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	1
	0.74
	170

	14
	[image: ]
	Unmarked batch #3
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	2
	0.81 ± 0.02
	174 ± 2

	15
	[image: ]
	Unmarked batch #4
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	1
	1.04
	234

	16
	[image: ]
	Unmarked batch #5
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	1
	0.73
	163

	17
	[image: ]
	Unmarked batch #6
	KN95
	flatfold
	GB2626-2006
	Not on Appendix A
	No
	Earloop straps
	1
	0.72
	164

	18
	[image: 3M(TM) Health Care Particulate Respirator and Surgical Mask 1860]
	3M 1860/1860S
	N95
	round
	NIOSH-42CFR84
	NIOSH N95 (FDA cleared)
	No
	Headband straps
	3
	1.43 ± 0.03
	316 ± 20

	19
	[image: 3M(TM) Particulate Respirator 8210, N95]
	3M 8210
	N95
	round
	NIOSH-42CFR84
	NIOSH N95 (FDA authorized)
	No
	Headband straps
	1
	1.43
	317

	20
	[image: 3M(TM) Aura(TM) Particulate Respirator 9210+, N95]
	3M 9210
	N95
	3 panel flatfold
	NIOSH-42CFR84
	NIOSH N95 (FDA authorized)
	No
	Headband straps
	1
	0.85
	168

	21
	[image: ]
	Cardinal Health ML/S
	N95
	round
	NIOSH-42CFR84
	NIOSH N95 (FDA cleared)
	No
	Headband straps
	5
	1.08 ± 0.12
	365 ± 28

	22
	[image: ]
	Gerson 1730
	N95
	round
	NIOSH-42CFR84
	NIOSH N95 (FDA cleared)
	No
	Headband straps
	1
	1.45
	328

	23
	[image: ]
	Kimberly-Clark 46767 (duckbill)
	N95
	duckbill
	NIOSH-42CFR84
	NIOSH N95 (FDA cleared)
	No
	Headband straps
	1
	0.66
	154

	24
	[image: ]
	Rizhao 3Q SanQi RIZSQ100Sb
	N95
	round
	NIOSH-42CFR84
	NIOSH N95 (FDA authorized)
	No
	Headband straps
	1
	1.18
	306

	25
	[image: ]
	San Huei SH9550
	N95
	round
	NIOSH-42CFR84
	NIOSH N95 (FDA authorized)
	No
	Headband straps
	1
	1.02
	306



*Each mask sample was measured three times.
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