Table 2: TWO Way Repeated ANOVA assessing the effect of material and thermocycling on Vickers Hardness (HV)
	Variables
	Df
	Mean Square
	F test
	P value
	Ƞ2

	Material
	1
	78.400
	81.215
	<.001
	0.819

	Thermocycling
	1
	78.400
	106.715
	<.001
	0.856

	Interaction
	1
	10.816
	14.722
	.001
	0.450


*Statistically significant difference at P<.05. Ƞ2: Partial Eta Squared

