Table The PM10, SO2, NO2, CO, and O3 concentration averaging periods and their limits in the Regulation on conditions for monitoring and air quality requirements  

	Air pollutant
	Concentration
	Averaging period
	Permitted exceedances

	Particulate matter (PM10) 
	50 µg/m3
	daily average
	35

	Particulate matter (PM10)
	40 µg/m3
	1 year average
	

	Sulphur dioxide (SO2)
	350 µg/m3
	1 hour average
	24

	Sulphur dioxide (SO2)
	125 µg/m3
	daily average
	3

	Sulphur dioxide (SO2)
	50 µg/m3
	1 year average
	

	Nitrogen dioxide (NO2)
	150 µg/m3
	1 hour average
	18

	Nitrogen dioxide (NO2)
	85 µg/m3
	daily average
	

	Nitrogen dioxide (NO2)
	40 µg/m3
	1 year average
	

	Carbon monoxide (CO)
	10 mg/m3
	maximum daily 8hrs average
	

	Carbon monoxide (CO)
	5 mg/m3
	daily average
	

	Ozone (O3)
	120 µg/m3
	maximum daily 8hrs average
	25 days averaged over



Suspended particles were in 2019 the dominant pollutant in the Republic of Serbia and exceedances of the daily limit values were at all measuring points. Exceedances of the yearly limit values were at 15 measuring points. Exceedances of the yearly limit values SO2 was only in Bor. Exceedances of the yearly limit values NO2 were only on two measuring points in Belgrade. Exceedances of the daily limit values CO were in Vranje and Zaječar. Exceedances of the target values O3 were at 16 measuring points, but exceedances of permitted number were only at two measuring points Kopaonik and Kamenički Vis-EMEP.
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