	Start protocol

	Command 
	Time (min)
	 Injection Port

	Calibrate
	 
	 

	Wait
	10
	 

	Mix
	1
	 

	Wait
	3
	 

	Mix
	1
	 

	Wait
	3
	 

	Mix
	1
	 

	Measure
	3
	 

	Mix
	1
	 

	Measure
	3
	 

	Mix
	1
	 

	Inject
	 
	A

	Mix
	1
	 

	Measure
	3
	 

	Mix
	1
	 

	Inject
	 
	B

	Mix
	1
	 

	Measure
	3
	 

	Mix
	1
	 

	Inject
	 
	C

	Mix
	1
	 

	Measure
	3
	 

	Mix
	1
	 

	Inject
	 
	D

	Mix
	1
	 

	Measure
	3
	 

	Mix
	1
	 


Table-S1: Instrument running protocol
























