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	Coil
	Sense breast 16-channel

	Matrix 
	400 x 400

	Pixel spacing (mm)
	0.8542

	Field of View (mm)
	3422

	In-plane resolution (mm)
	0.92

	Repetition time (msec)
	2000

	Echo time (msec)
	218

	Flip angle (°)
	90

	Echo train length
	95

	Slice thickness (mm)
	2.0






