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S1
The purity of the title compounds
The purity of the title compounds was determined using an Agilent 1260 HPLC equipped with an Eclipse XDB C18 chromatographic column. The temperature was held at 303.15 K during the analytical procedure. The wavelength of the ultraviolet detector was set to 230 nm and the sample injection volume was 5 μL. The mobile phase was methanol/water (90/10), injected at a flow rate of 0.4 mL·min−1. The results were shown in Figure 2 and 3.
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[bookmark: _GoBack]Fig.1 The crystal of 1,1ʹ-azobis-1,2,3-triazole (1) and 4,4ʹ-azobis-1,2,4-triazole (2)
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[bookmark: OLE_LINK1]Fig.2 High-performance liquid chromatograph (HLPC) of 1
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Fig.3 High-performance liquid chromatograph (HLPC) of 2
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