	Camera System
	Field of View
	Blind Spot Risk
	Detection Accuracy
	Cost Level
	Deployment Suitability

	Narrow Webcam
	Limited
	High
	97.73% (conventional)
	Low
	Corporate cost-efficient

	Fisheye
	180°–360°
	Moderate
	71.06%
	Medium
	Wide-area coverage

	Multi-camera
	Distributed
	Low
	94.6%
	High
	Critical security zones
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