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	PET system
	Matrix size
	Contrast (%)
	CV (%)
	SD           (Clinical vs. 30 min)

	PMT-PET
	128 × 128
	58.5
	11.1
	0.021/0.018

	PMT-PET
	256 × 256
	58.5
	10.5
	0.021/0.018

	SiPM-PET
	128 × 128
	72.4
	11.5
	0.015/0.009

	SiPM-PET
	256 × 256
	72.8
	10.9
	0.016/0.009


CV, coefficient of variation; PET, positron emission tomography; PMT, photomultiplier tube; SD, standard deviation; SiPM, silicon photomultiplier.
